,Weight Product##OTHER##,Trim##OTHER##,Transformer Taps##OTHER##,Transducers (LF/HF)##OTHER##,System Sensitivity  (1W @ 1m)##OTHER##,Shipping Weight##OTHER##,Sensitivity##OTHER##,Safety Agency Rating##OTHER##,Rotation Offset##ANGLE##DECIMAL DEGREES,Rotation##ANGLE##DECIMAL DEGREES,Recommeded Amplifier Power##OTHER##,Rated Maximum SPL (Max Transformer Tap)##OTHER##,Rated Maximum SPL (Avg/Peak)##OTHER##,REP##OTHER##,Product Page URL##OTHER##,Product Documentation Link##OTHER##,Power Handling - Program##OTHER##,Power Handling - Peak##OTHER##,Power Handling - Avg##OTHER##,Peak Factor##OTHER##,Packed Qty##OTHER##,Optional Accessories##OTHER##,Operating Temperature##OTHER##,Nominal Impedance##OTHER##,Nominal Coverage Angle  (HxV -6dB)##OTHER##,Model##OTHER##,Manufacturer##OTHER##,Logo##OTHER##,Input Connector##OTHER##,Included Accessories##OTHER##,Hardware Finish##OTHER##,Grille Material##OTHER##,Grill Scrim##OTHER##,Grill Finish##OTHER##,Frequency Response (+/- 3dB)##OTHER##,Frequency  Range (-10dB)##OTHER##,Environmental Testing##OTHER##,Environmental##OTHER##,Enclosure##OTHER##,Directivity Index (dB)##OTHER##,Desired Level @ Listener##OTHER##,Description##OTHER##,Default Elevation##LENGTH##FEET,D2##LENGTH##FEET,Case Finish 2##OTHER##,Case Finish##OTHER##,Azimuth Offset##ANGLE##DECIMAL DEGREES,Azimuth##ANGLE##DECIMAL DEGREES,AS-8T##OTHER##,AS-5T##OTHER##,AS-4T##OTHER##,AS-6T##OTHER##,AS-10T##OTHER##
AS-4T-B,5.93,"Laminate, Black, Matte","15W, 7.5W, 3.8W ( 1.9W 70V) & Low Z operation","LF: 4"" (100mm) Polypropylene, Butyl Rubber surround, HF: 1"" (25mm), Silk Dome, Ferrofluid Cooled, PPT Protection",86dB,18.28,86,"UL1480A, CE",90.000000000000,0.000000000000,80W @ 8 Ohms,98dB,102/108 dB,29.53426,https://www.atlasied.com/as-4t,,80W,160W,40W,10,2,Pan & Tilt Bracket,-40°F to 140°F (-40° C to 60° C),8 Ohms (Min 6.8 Ohms),140° x 140°,AS-4T-B,AtlasIED,"Laminate, Black, Matte",Euroblock with screw connections and loop output,Slip Free U-Bracket,"Metal, Powder Coated, Black","Aluminium, Powder Coated",Grille Scrim - Black,Black Grille,107Hz-20kHz,73Hz-20kHz,Conforms to MIL-STD-810 for salt spray & humidity,IP55,High Impact ABS UL-V0,5.9,75,"4"" Surface Mount, Passive, Black",4.000000000000,20.000000000000,"Laminate, Black, Matte","Laminate, Black, Matte",90.000000000000,0.000000000000,0,0,1,0,0
AS-4T-W,5.93,"Laminate, White, Matte","15W, 7.5W, 3.8W ( 1.9W 70V) & Low Z operation","LF: 4"" (100mm) Polypropylene, Butyl Rubber surround, HF: 1"" (25mm), Silk Dome, Ferrofluid Cooled, PPT Protection",86dB,18.28,86,"UL1480A, CE",90.000000000000,0.000000000000,80W @ 8 Ohms,98dB,102/108 dB,29.53426,https://www.atlasied.com/as-4t,,80W,160W,40W,10,2,Pan & Tilt Bracket,-40°F to 140°F (-40° C to 60° C),8 Ohms (Min 6.8 Ohms),140° x 140°,AS-4T-B,AtlasIED,"Laminate, White, Matte",Euroblock with screw connections and loop output,Slip Free U-Bracket,Steel - White Powder coated,"Aluminium, Powder Coated",Grille Scrim - White,White Grille,107Hz-20kHz,73Hz-20kHz,Conforms to MIL-STD-810 for salt spray & humidity,IP55,High Impact ABS UL-V0,5.9,75,"4"" Surface Mount, Passive, White",4.000000000000,20.000000000000,"Laminate, White, Matte","Laminate, White, Matte",90.000000000000,0.000000000000,0,0,1,0,0
AS-5T-W,9.28,"Laminate, White, Matte","30W, 15W, 7.5W, 3.8W ( 1.9W 70V) & Low Z operation","LF: 5.25"" (130mm) Polypropylene, Butyl Rubber surround, HF: 1"" (25mm), Silk Dome, Ferrofluid Cooled, PPT Protection",87dB,27.34,87,"UL1480A, CE",90.000000000000,0.000000000000,200W @ 8 Ohms,102dB,107/113 dB,23.459897,https://www.atlasied.com/as-5t,,200W,400W,100W,10,2,Pan & Tilt Bracket,-40°F to 140°F (-40° C to 60° C),8 Ohms (Min 7.4 Ohms),120° x 120°,AS-5T-W,AtlasIED,"Laminate, White, Matte",Euroblock with screw connections and loop output,Slip Free U-Bracket,Steel - White Powder coated,"Aluminium, Powder Coated",Grille Scrim - White,White Grille,95Hz-20kHz,63Hz-20kHz,Conforms to MIL-STD-810 for salt spray & humidity,IP55,High Impact ABS UL-V0,7.3,75,"5.25"" Surface Mount, Passive, White",4.000000000000,20.000000000000,"Laminate, White, Matte","Laminate, White, Matte",90.000000000000,0.000000000000,0,1,0,0,0
AS-5T-B,9.28,"Laminate, Black, Matte","30W, 15W, 7.5W, 3.8W ( 1.9W 70V) & Low Z operation","LF: 5.25"" (130mm) Polypropylene, Butyl Rubber surround, HF: 1"" (25mm), Silk Dome, Ferrofluid Cooled, PPT Protection",87dB,27.34,87,"UL1480A, CE",90.000000000000,0.000000000000,200W @ 8 Ohms,102dB,107/113 dB,23.459897,https://www.atlasied.com/as-5t,,200W,400W,100W,10,2,Pan & Tilt Bracket,-40°F to 140°F (-40° C to 60° C),8 Ohms (Min 7.4 Ohms),120° x 120°,AS-5T-B,AtlasIED,"Laminate, Black, Matte",Euroblock with screw connections and loop output,Slip Free U-Bracket,"Metal, Powder Coated, Black","Aluminium, Powder Coated",Grille Scrim - Black,Black Grille,95Hz-20kHz,63Hz-20kHz,Conforms to MIL-STD-810 for salt spray & humidity,IP55,High Impact ABS UL-V0,7.3,75,"5.25"" Surface Mount, Passive, Black",4.000000000000,20.000000000000,"Laminate, Black, Matte","Laminate, Black, Matte",90.000000000000,0.000000000000,0,1,0,0,0
AS-6T-B,13,"Laminate, Black, Matte","60W, 30W, 15W, 7.5W,( 3.8W 70V) & Low Z operation","LF: 6"" (150mm) Polypropylene, Butyl Rubber surround, HF: 1.25"" (32mm), Silk Dome, Ferrofluid Cooled, PPT Protection",88dB,43.8,88,"UL1480A, CE",90.000000000000,0.000000000000,300W @ 8 Ohms,106dB,110/116 dB,18.634858,https://www.atlasied.com/as-6t,,300W,600W,150W,10,2,Pan & Tilt Bracket,-40°F to 140°F (-40° C to 60° C),8 Ohms (Min 7.4 Ohms),110° x 90°,AS-6T-B,AtlasIED,"Laminate, Black, Matte",Euroblock with screw connections and loop output,Slip Free U-Bracket,"Metal, Powder Coated, Black","Aluminium, Powder Coated",Grille Scrim - Black,Black Grille,74Hz-20kHz,"55Hz-20kHz
55Hz-20kHz",Conforms to MIL-STD-810 for salt spray & humidity,IP55,High Impact ABS UL-V0,6.6,75,"6.5"" Surface Mount, Passive, Black",4.000000000000,20.000000000000,"Laminate, Black, Matte","Laminate, Black, Matte",90.000000000000,0.000000000000,0,0,0,1,0
AS-6T-W,13,"Laminate, White, Matte","60W, 30W, 15W, 7.5W,( 3.8W 70V) & Low Z operation","LF: 6"" (150mm) Polypropylene, Butyl Rubber surround, HF: 1.25"" (32mm), Silk Dome, Ferrofluid Cooled, PPT Protection",88dB,43.8,88,"UL1480A, CE",90.000000000000,0.000000000000,300W @ 8 Ohms,106dB,110/116 dB,18.634858,https://www.atlasied.com/as-6t,,300W,600W,150W,10,2,Pan & Tilt Bracket,-40°F to 140°F (-40° C to 60° C),8 Ohms (Min 7.4 Ohms),110° x 90°,AS-6T-W,AtlasIED,"Laminate, White, Matte",Euroblock with screw connections and loop output,Slip Free U-Bracket,Steel - White Powder coated,"Aluminium, Powder Coated",Grille Scrim - White,White Grille,74Hz-20kHz,"55Hz-20kHz
55Hz-20kHz",Conforms to MIL-STD-810 for salt spray & humidity,IP55,High Impact ABS UL-V0,6.6,75,"6.5"" Surface Mount, Passive, White",4.000000000000,20.000000000000,"Laminate, White, Matte","Laminate, White, Matte",90.000000000000,0.000000000000,0,0,0,1,0
AS-8T-B,23.9,"Laminate, Black, Matte","60W, 30W, 15W, 7.5W,( 3.8W 70V) & Low Z operation","LF: 8"" (200mm"") Weather Treated Paper,Butyl Rubber Surround, HF: 25 mm (1 in) Exit Compression Driver, PPT Protection",90,31.31,90,"UL1480A, CE",90.000000000000,0.000000000000,360W @ 8 Ohms,108dB,113/119 dB,11.757801,https://www.atlasied.com/as-8t,,360W,720W,180W,10,2,,-40°F to 140°F (-40° C to 60° C),8 Ohms (Min 7.4 Ohms),110° x 90°,AS-8T-B,AtlasIED,"Laminate, Black, Matte",Euroblock with screw connections and loop output,Slip Free U-Bracket,"Metal, Powder Coated, Black","Aluminium, Powder Coated",Grille Scrim - Black,Black Grille,70Hz-18kHz,49Hz-20kHz,Conforms to MIL-STD-810 for salt spray & humidity,IP55,High Impact ABS UL-V0,8.2,75,"8"" Surface Mount, Passive, Black",4.000000000000,20.000000000000,"Laminate, Black, Matte","Laminate, Black, Matte",90.000000000000,0.000000000000,1,0,0,0,0
AS-8T-W,23.9,"Laminate, White, Matte","60W, 30W, 15W, 7.5W,( 3.8W 70V) & Low Z operation","LF: 8"" (200mm"") Weather Treated Paper,Butyl Rubber Surround, HF: 25 mm (1 in) Exit Compression Driver, PPT Protection",90,31.31,90,"UL1480A, CE",90.000000000000,0.000000000000,360W @ 8 Ohms,108dB,113/119 dB,11.757801,https://www.atlasied.com/as-8t,,360W,720W,180W,10,2,,-40°F to 140°F (-40° C to 60° C),8 Ohms (Min 7.4 Ohms),110° x 90°,AS-8T-W,AtlasIED,"Laminate, White, Matte",Euroblock with screw connections and loop output,Slip Free U-Bracket,Steel - White Powder coated,"Aluminium, Powder Coated",Grille Scrim - White,White Grille,70Hz-18kHz,49Hz-20kHz,Conforms to MIL-STD-810 for salt spray & humidity,IP55,High Impact ABS UL-V0,8.2,75,"8"" Surface Mount, Passive, White",4.000000000000,20.000000000000,"Laminate, White, Matte","Laminate, White, Matte",90.000000000000,0.000000000000,1,0,0,0,0
AS-10T-B,35.63,"Laminate, Black, Matte","60W, 30W, 15W, 7.5W,( 3.8W 70V) & Low Z operation","LF: 8"" (200mm"") Weather Treated Paper,Butyl Rubber Surround, HF: 25 mm (1 in) Exit Compression Driver, PPT Protection",90,31.31,90,"UL1480A, CE",90.000000000000,0.000000000000,4800W @ 8 Ohms,114dB,117/123dB,11.757801,https://www.atlasied.com/as-10t,,480W,960W,240W,10,2,,-40°F to 140°F (-40° C to 60° C),8 Ohms (Min 7.4 Ohms),110° x 90°,AS-10T-B,AtlasIED,"Laminate, Black, Matte",Euroblock with screw connections and loop output,Slip Free U-Bracket,"Metal, Powder Coated, Black","Aluminium, Powder Coated",Grille Scrim - Black,Black Grille,58Hz-18kHz,45Hz-20kHz,Conforms to MIL-STD-810 for salt spray & humidity,IP55,High Impact ABS UL-V0,8.5,75,"10"" Surface Mount, Passive, Black",4.000000000000,20.000000000000,"Laminate, Black, Matte","Laminate, Black, Matte",90.000000000000,0.000000000000,0,0,0,0,1
AS-10ST-B,49.16,"Laminate, Black, Matte","60W, 30W, 15W, 7.5W,( 3.8W 70V) & Low Z operation","LF: 8"" (200mm"") Weather Treated Paper,Butyl Rubber Surround, HF: 25 mm (1 in) Exit Compression Driver, PPT Protection",90,35.27,90,"UL1480A, CE",90.000000000000,0.000000000000,600W @ 8 Ohms,116dB,118/124dB,11.757801,https://www.atlasied.com/as-10t,,600W,1200W,300W,10,2,,-40°F to 140°F (-40° C to 60° C),4 Ohms (Min 7.4 Ohms),Omni,AS-10ST-B,AtlasIED,"Laminate, Black, Matte",Euroblock with screw connections and loop output,Slip Free U-Bracket,"Metal, Powder Coated, Black","Aluminium, Powder Coated",Grille Scrim - Black,Black Grille,43Hz-600Hz,34Hz-800Hz,Conforms to MIL-STD-810 for salt spray & humidity,IP55,High Impact ABS UL-V0,N/A,75,"10"" Surface Mount Direct Radiating Subwoofer, Black",4.000000000000,20.000000000000,"Laminate, Black, Matte","Laminate, Black, Matte",90.000000000000,0.000000000000,0,0,0,0,1
AS-10ST-W,49.16,"Laminate, White, Matte","60W, 30W, 15W, 7.5W,( 3.8W 70V) & Low Z operation","LF: 8"" (200mm"") Weather Treated Paper,Butyl Rubber Surround, HF: 25 mm (1 in) Exit Compression Driver, PPT Protection",90,35.27,90,"UL1480A, CE",90.000000000000,0.000000000000,600W @ 8 Ohms,116dB,118/124dB,11.757801,https://www.atlasied.com/as-10t,,600W,1200W,300W,10,2,,-40°F to 140°F (-40° C to 60° C),4 Ohms (Min 7.4 Ohms),Omni,AS-10ST-W,AtlasIED,"Laminate, White, Matte",Euroblock with screw connections and loop output,Slip Free U-Bracket,Steel - White Powder coated,"Aluminium, Powder Coated",Grille Scrim - White,White Grille,43Hz-600Hz,34Hz-800Hz,Conforms to MIL-STD-810 for salt spray & humidity,IP55,High Impact ABS UL-V0,N/A,75,"10"" Surface Mount Direct Radiating Subwoofer, White",4.000000000000,20.000000000000,"Laminate, White, Matte","Laminate, White, Matte",90.000000000000,0.000000000000,0,0,0,0,1
AS-10T-W,35.63,"Laminate, White, Matte","60W, 30W, 15W, 7.5W,( 3.8W 70V) & Low Z operation","LF: 8"" (200mm"") Weather Treated Paper,Butyl Rubber Surround, HF: 25 mm (1 in) Exit Compression Driver, PPT Protection",90,31.31,90,"UL1480A, CE",90.000000000000,0.000000000000,4800W @ 8 Ohms,114dB,117/123dB,11.757801,https://www.atlasied.com/as-10t,,480W,960W,240W,10,2,,-40°F to 140°F (-40° C to 60° C),8 Ohms (Min 7.4 Ohms),110° x 90°,AS-10T-W,AtlasIED,"Laminate, White, Matte",Euroblock with screw connections and loop output,Slip Free U-Bracket,Steel - White Powder coated,"Aluminium, Powder Coated",Grille Scrim - White,White Grille,58Hz-18kHz,45Hz-20kHz,Conforms to MIL-STD-810 for salt spray & humidity,IP55,High Impact ABS UL-V0,8.5,75,"10"" Surface Mount, Passive, White",4.000000000000,20.000000000000,"Laminate, White, Matte","Laminate, White, Matte",90.000000000000,0.000000000000,0,0,0,0,1
