,Weight Product##OTHER##,URL##OTHER##,Trim##OTHER##,Transformer Taps##OTHER##,Transducers (LF/HF)##OTHER##,Tile Bridge Spacing##LENGTH##FEET,System Sensitivity  (1W @ 1m)##OTHER##,Square Grille##OTHER##,Shipping Weight##OTHER##,Shipping Dimensions (HxWxD)##OTHER##,Sensitivity##OTHER##,Safety Agency Rating##OTHER##,Round Grille##OTHER##,Recommeded Amplifier Power##OTHER##,Rated Maximum SPL (Max Transformer Tap)##OTHER##,Rated Maximum SPL (Avg/Peak)##OTHER##,REP##OTHER##,Product Page URL##OTHER##,Product Documentation Link##OTHER##,Power Handling - Program##OTHER##,Power Handling - Peak##OTHER##,Power Handling - Avg##OTHER##,Peak Factor##OTHER##,Packed Qty##OTHER##,Optional Accessories##OTHER##,Operating Temperature##OTHER##,Nominal Impedance##OTHER##,Nominal Coverage Angle  (HxV -6dB)##OTHER##,Model##OTHER##,Minimum Overlap Spacing##LENGTH##FEET,Min Tap Value##OTHER##,Min Overlap Guide##OTHER##,Manufacturer##OTHER##,Listener Height##OTHER##,Input Connector##OTHER##,Included Accessories##OTHER##,Include Tile Bridge##OTHER##,Include C Ring##OTHER##,Grille Material##OTHER##,Grille Diameter##OTHER##,Grill Scrim##OTHER##,Grill Finish##OTHER##,Front of ceiling to top of safety loop##OTHER##,Front of ceiling to rear of backcan##OTHER##,Frequency Response (+/- 3dB)##OTHER##,Frequency  Range (-10dB)##OTHER##,FC-8TPI##OTHER##,FC-8T##OTHER##,FC-6TPI##OTHER##,FC-6T##OTHER##,FC-4TLP##OTHER##,FC-4T##OTHER##,Environmental Testing##OTHER##,Environmental##OTHER##,Enclosure##OTHER##,Edge-To-Edge Spacing##LENGTH##FEET,Edge-To-Edge Guide##OTHER##,Dispersion##OTHER##,Directivity Index (dB)##OTHER##,Desired Level @ Listener##OTHER##,Description##OTHER##,Depth##LENGTH##FEET,Default Elevation##LENGTH##FEET,Cutout Diameter##OTHER##,Conduit Knockouts on PI Backcan##OTHER##,Ceiling Height##OTHER##,Case Finish##OTHER##,Black Round Grille##OTHER##,Bezel Diameter##OTHER##,30W XFRM##OTHER##
FC-4T - White,7.9,https://www.atlasied.com,"Laminate, White, Matte","30W, 15W, 7.5W, 3.8W ( 1.9W 70V) & Low Z operation","LF: 4"" (100mm)  Bass/Mid, mineral loaded polypropylene, HF: 0.75"" (19mm) titanium dome with neodymium magnet system, Ferrofluid cooled",0.437500000000,88dB,0,25.9,11.8"" x 28"" x 14.6"" (30cm x 71cm x 37cm),90.1,"UL1480A, UL2043, CE",1,120W @ 8 Ohms,104dB,106/112 dB,1.034082,https://www.atlasied.com/fc-4t,,120W,240W,60W,10,2,"Round black grill, square white grill, square black grill",-40°F to 140°F (-40° C to 60° C),8 Ohms,100°,FC-4T,10.725782333348,3.8,0,AtlasIED,6,Removable locking dinkle connector with screw terminals & loop through facility,"C-Ring, tile-bridge kit, cut-out template, round white grille",1,1,"Steel, weather resistent coating (White)",Ø8.78"" (223mm),Grill Scrim,White Grille,8.91"" (226.5mm),8.13"" (206.5mm),84Hz-22kHz,64Hz-30kHz,0,0,0,0,0,1,Salt Spray & Chlorine,IP33,"Backcan: Powder Coated Steel (Black), Baffle: High Impact ABS UL-V0 (Black), Grille: Steel, weather resistent coating (White)",14.301043111130,0,100,4.7,75,4"" Premium Ceiling Speaker (Blind Mount) - White,0.742513020833,4.000000000000,Ø 7.56"" (192mm),,12,Steel - Black Powder coated,0,Ø 8.42"" (213.9mm),1
FC-4T - Black,7.9,https://www.atlasied.com,"Laminate, Black","30W, 15W, 7.5W, 3.8W ( 1.9W 70V) & Low Z operation","LF: 4"" (100mm)  Bass/Mid, mineral loaded polypropylene, HF: 0.75"" (19mm) titanium dome with neodymium magnet system, Ferrofluid cooled",0.437500000000,88dB,0,25.9,11.8"" x 28"" x 14.6"" (30cm x 71cm x 37cm),90.1,"UL1480A, UL2043, CE",1,120W @ 8 Ohms,104dB,106/112 dB,1.034082,https://www.atlasied.com/fc-4t,,120W,240W,60W,10,2,"Round black grill, square white grill, square black grill",-40°F to 140°F (-40° C to 60° C),8 Ohms,100°,FC-4T,10.725782333348,3.8,0,AtlasIED,6,Removable locking dinkle connector with screw terminals & loop through facility,"C-Ring, tile-bridge kit, cut-out template, round white grille",1,1,"Steel, weather resistent coating (White)",Ø8.78"" (223mm),Grille Scrim - Black,Black Grille,8.91"" (226.5mm),8.13"" (206.5mm),84Hz-22kHz,64Hz-30kHz,0,0,0,0,0,1,Salt Spray & Chlorine,IP33,"Backcan: Powder Coated Steel (Black), Baffle: High Impact ABS UL-V0 (Black), Grille: Steel, weather resistent coating (White)",14.301043111130,0,100,4.7,75,4"" Premium Ceiling Speaker (Blind Mount) - Black,0.742513020833,4.000000000000,Ø 7.56"" (192mm),,12,Steel - Black Powder coated,0,Ø 8.42"" (213.9mm),1
FC-4TLP - Black,7.9,https://www.atlasied.com,"Laminate, Black","30W, 15W, 7.5W, 3.8W ( 1.9W 70V) & Low Z operation","LF: 4"" (100mm)  Bass/Mid, mineral loaded polypropylene, HF: 0.75"" (19mm) titanium dome with neodymium magnet system, Ferrofluid cooled",0.674804687500,88dB,0,25.9,11.8"" x 28"" x 14.6"" (30cm x 71cm x 37cm),90.1,"UL1480A, UL2043, CE",1,120W @ 8 Ohms,104dB,106/112 dB,1.034082,https://www.atlasied.com/fc-4tlp,,120W,240W,60W,10,2,"Round black grill, square white grill, square black grill",-40°F to 140°F (-40° C to 60° C),8 Ohms,100°,FC-4TLP,10.725782333348,3.8,0,AtlasIED,6,Removable locking dinkle connector with screw terminals & loop through facility,"C-Ring, tile-bridge kit, cut-out template, round white grille",1,1,"Steel, weather resistent coating (White)",Ø11.18"" (284mm),Grille Scrim - Black,Black Grille,,(3.96"") 100.5mm,84Hz-22kHz,64Hz-30kHz,0,0,0,0,1,0,Salt Spray & Chlorine,IP33,"Backcan: Powder Coated Steel (Black), Baffle: High Impact ABS UL-V0 (Black), Grille: Steel, weather resistent coating (White)",14.301043111130,0,100,4.7,75,4"" Premium Low Profile Ceiling Speaker (Blind Mount) - Black,0.330078125000,4.000000000000,Ø 9.76"" (248mm),,12,Steel - Black Powder coated,0,Ø  10.83"" (275.1mm),1
FC-4TLP - White,7.9,https://www.atlasied.com,"Laminate, White, Matte","30W, 15W, 7.5W, 3.8W ( 1.9W 70V) & Low Z operation","LF: 4"" (100mm)  Bass/Mid, mineral loaded polypropylene, HF: 0.75"" (19mm) titanium dome with neodymium magnet system, Ferrofluid cooled",0.674804687500,88dB,0,25.9,11.8"" x 28"" x 14.6"" (30cm x 71cm x 37cm),90.1,"UL1480A, UL2043, CE",1,120W @ 8 Ohms,104dB,106/112 dB,1.034082,https://www.atlasied.com/fc-4tlp,,120W,240W,60W,10,2,"Round black grill, square white grill, square black grill",-40°F to 140°F (-40° C to 60° C),8 Ohms,100°,FC-4TLP,10.725782333348,3.8,0,AtlasIED,6,Removable locking dinkle connector with screw terminals & loop through facility,"C-Ring, tile-bridge kit, cut-out template, round white grille",1,1,"Steel, weather resistent coating (White)",Ø11.18"" (284mm),Grille Scrim - White,White Grille,,(3.96"") 100.5mm,84Hz-22kHz,64Hz-30kHz,0,0,0,0,1,0,Salt Spray & Chlorine,IP33,"Backcan: Powder Coated Steel (Black), Baffle: High Impact ABS UL-V0 (Black), Grille: Steel, weather resistent coating (White)",14.301043111130,0,100,4.7,75,4"" Premium Low Profile Ceiling Speaker (Blind Mount) - White,0.330078125000,4.000000000000,Ø 9.76"" (248mm),,12,Steel - Black Powder coated,0,Ø  10.83"" (275.1mm),1
FC-6T - White,13.2,https://www.atlasied.com,"Laminate, White, Matte","30W, 15W, 7.5W, 3.8W ( 1.9W 70V) & Low Z operation","LF: (6"") 150mm Bass/Mid, mineral loaded polypropylene, HF: 1"" (25mm) titanium dome with neodymium magnet system, Ferrofluid cooled",0.593750000000,91dB,0,39.6,14.6"" x 33.7"" x 18.1"" (37cm x 85.5cm x 46cm),91,"UL1480A, UL2043, CE",1,160W @ 8 Ohms,109dB,110/116 dB,0.840533,https://www.atlasied.com/fc-6t,,160W,320W,80W,10,2,"Round black grill, square white grill, square black grill",-40°F to 140°F (-40° C to 60° C),8 Ohms,100°,FC-6T,10.725782333348,7.5,0,AtlasIED,6,Removable locking dinkle connector with screw terminals & loop through facility,"C-Ring, tile-bridge kit, cut-out template, round white grille",1,1,"Steel, weather resistent coating (White)",Ø11.18"" (284mm),Grille Scrim - White,White Grille,294mm (11.55""),273.5mm (10.76""),65Hz-25kHz,48Hz-30kHz,0,0,0,1,0,0,Salt Spray & Chlorine,IP33,"Backcan: Powder Coated Steel (Black), Baffle: High Impact ABS UL-V0 (Black), Grille: Steel, weather resistent coating (White)",14.301043111130,0,100,5.6,75,6"" Premium Ceiling Speaker (Blind Mount) - White,0.962565104167,4.000000000000,Ø 9.76"" (248mm),,12,Steel - Black Powder coated,0,Ø  10.83"" (275.1mm),0
FC-6T - Black,13.2,https://www.atlasied.com,"Laminate, Black","30W, 15W, 7.5W, 3.8W ( 1.9W 70V) & Low Z operation","LF: (6"") 150mm Bass/Mid, mineral loaded polypropylene, HF: 1"" (25mm) titanium dome with neodymium magnet system, Ferrofluid cooled",0.593750000000,91dB,0,39.6,14.6"" x 33.7"" x 18.1"" (37cm x 85.5cm x 46cm),91,"UL1480A, UL2043, CE",1,160W @ 8 Ohms,109dB,110/116 dB,0.840533,https://www.atlasied.com/fc-6t,,160W,320W,80W,10,2,"Round black grill, square white grill, square black grill",-40°F to 140°F (-40° C to 60° C),8 Ohms,100°,FC-6T,10.725782333348,7.5,0,AtlasIED,6,Removable locking dinkle connector with screw terminals & loop through facility,"C-Ring, tile-bridge kit, cut-out template, round white grille",1,1,"Steel, weather resistent coating (White)",Ø11.18"" (284mm),Grille Scrim - Black,Black Grille,294mm (11.55""),273.5mm (10.76""),65Hz-25kHz,48Hz-30kHz,0,0,0,1,0,0,Salt Spray & Chlorine,IP33,"Backcan: Powder Coated Steel (Black), Baffle: High Impact ABS UL-V0 (Black), Grille: Steel, weather resistent coating (White)",14.301043111130,0,100,5.6,75,6"" Premium Ceiling Speaker (Blind Mount) - White,0.962565104167,4.000000000000,Ø 9.76"" (248mm),,12,Steel - Black Powder coated,0,Ø  10.83"" (275.1mm),0
FC-8TPI - Black,13.2,https://www.atlasied.com,"Laminate, Black","30W, 15W, 7.5W, 3.8W ( 1.9W 70V) & Low Z operation","LF: (8"") 200mm Bass/Mid, mineral loaded polypropylene, HF: 1"" (25mm) titanium dome with neodymium magnet system, Ferrofluid cooled",0.677083333333,91dB,0,52,16.2"" x 37.4"" x 22.1"" (41cm x 95cm x 56cm),91,"UL1480A, UL2043, CE",1,160W @ 8 Ohms,109dB,110/116 dB,0.840533,https://www.atlasied.com/fc-8tpi,,160W,320W,80W,10,2,"Round black grill, square white grill, square black grill",-40°F to 140°F (-40° C to 60° C),8 Ohms,90°,FC-8TPI,9.000000000000,7.5,0,AtlasIED,6,Removable locking dinkle connector with screw terminals & loop through facility,"C-Ring, tile-bridge kit, cut-out template, round white grille",1,1,"Steel, weather resistent coating (Black)",Ø13.07"" (332mm),Grille Scrim - Black,Black Grille,13.42"" (341mm),12.63"" (321mm),77Hz-19kHz,58Hz-20kHz,1,0,0,0,0,0,Salt Spray & Chlorine,IP33,"Backcan: Powder Coated Steel (Black), Baffle: High Impact ABS UL-V0 (Black), Grille: Steel, weather resistent coating (Black)",12.000000000000,0,90,7.5,75,8"" Premium Ceiling Speaker (Pre-Install) - Black,1.118489583333,4.000000000000,Ø 11.57"" (294mm),7 locations  -     0.75/0.87/1.10"" (19/22/28mm),12,Steel - Black Powder coated,0,Ø 12.75"" (323.9mm),0
FC-6TPI - White,13.2,https://www.atlasied.com,"Laminate, White, Matte","30W, 15W, 7.5W, 3.8W ( 1.9W 70V) & Low Z operation","LF: (6"") 150mm Bass/Mid, mineral loaded polypropylene, HF: 1"" (25mm) titanium dome with neodymium magnet system, Ferrofluid cooled",0.593750000000,91dB,1,39.6,14.6"" x 33.7"" x 18.1"" (37cm x 85.5cm x 46cm),91,"UL1480A, UL2043, CE",0,160W @ 8 Ohms,109dB,110/116 dB,0.840533,https://www.atlasied.com/fc-6tpi,,160W,320W,80W,10,2,"Round black grill, square white grill, square black grill",-40°F to 140°F (-40° C to 60° C),8 Ohms,100°,FC-6TPI,10.725782333348,7.5,0,AtlasIED,6,Removable locking dinkle connector with screw terminals & loop through facility,"C-Ring, tile-bridge kit, cut-out template, round white grille",1,1,"Steel, weather resistent coating (White)",Ø11.18"" (284mm),Grille Scrim - White,White Grille,294mm (11.55""),273.5mm (10.76""),65Hz-25kHz,48Hz-30kHz,0,0,1,0,0,0,Salt Spray & Chlorine,IP33,"Backcan: Powder Coated Steel (Black), Baffle: High Impact ABS UL-V0 (Black), Grille: Steel, weather resistent coating (White)",14.301043111130,0,100,5.6,75,6"" Premium Ceiling Speaker (Pre-Install) - White,0.962565104167,4.000000000000,Ø 9.76"" (248mm),5 locations  -     0.5/0.75/0.87/1.10"" (12.7/19/22/28mm),12,Steel - Black Powder coated,0,Ø  10.83"" (275.1mm),0
FC-6TPI - Black,13.2,https://www.atlasied.com,"Laminate, Black","30W, 15W, 7.5W, 3.8W ( 1.9W 70V) & Low Z operation","LF: (6"") 150mm Bass/Mid, mineral loaded polypropylene, HF: 1"" (25mm) titanium dome with neodymium magnet system, Ferrofluid cooled",0.593750000000,91dB,0,39.6,14.6"" x 33.7"" x 18.1"" (37cm x 85.5cm x 46cm),91,"UL1480A, UL2043, CE",1,160W @ 8 Ohms,109dB,110/116 dB,0.840533,https://www.atlasied.com/fc-6tpi,,160W,320W,80W,10,2,"Round black grill, square white grill, square black grill",-40°F to 140°F (-40° C to 60° C),8 Ohms,100°,FC-6TPI,10.725782333348,7.5,0,AtlasIED,6,Removable locking dinkle connector with screw terminals & loop through facility,"C-Ring, tile-bridge kit, cut-out template, round white grille",1,1,"Steel, weather resistent coating (White)",Ø11.18"" (284mm),Grille Scrim - Black,Black Grille,294mm (11.55""),273.5mm (10.76""),65Hz-25kHz,48Hz-30kHz,0,0,1,0,0,0,Salt Spray & Chlorine,IP33,"Backcan: Powder Coated Steel (Black), Baffle: High Impact ABS UL-V0 (Black), Grille: Steel, weather resistent coating (White)",14.301043111130,0,100,5.6,75,6"" Premium Ceiling Speaker (Pre-Install) - Black,0.962565104167,4.000000000000,Ø 9.76"" (248mm),5 locations  -     0.5/0.75/0.87/1.10"" (12.7/19/22/28mm),12,Steel - Black Powder coated,0,Ø  10.83"" (275.1mm),0
FC-8T - White,13.2,https://www.atlasied.com,"Laminate, White, Matte","30W, 15W, 7.5W, 3.8W ( 1.9W 70V) & Low Z operation","LF: (8"") 200mm Bass/Mid, mineral loaded polypropylene, HF: 1"" (25mm) titanium dome with neodymium magnet system, Ferrofluid cooled",0.677083333333,91dB,0,52,16.2"" x 37.4"" x 22.1"" (41cm x 95cm x 56cm),91,"UL1480A, UL2043, CE",1,160W @ 8 Ohms,109dB,110/116 dB,0.840533,https://www.atlasied.com/fc-8t,,160W,320W,80W,10,2,"Round black grill, square white grill, square black grill",-40°F to 140°F (-40° C to 60° C),8 Ohms,90°,FC-8T,9.000000000000,7.5,0,AtlasIED,6,Removable locking dinkle connector with screw terminals & loop through facility,"C-Ring, tile-bridge kit, cut-out template, round white grille",1,1,"Steel, weather resistent coating (Black)",Ø13.07"" (332mm),Grille Scrim - White,White Grille,13.42"" (341mm),12.63"" (321mm),77Hz-19kHz,58Hz-20kHz,0,1,0,0,0,0,Salt Spray & Chlorine,IP33,"Backcan: Powder Coated Steel (Black), Baffle: High Impact ABS UL-V0 (White), Grille: Steel, weather resistent coating (White)",12.000000000000,0,90,7.5,75,8"" Premium Ceiling Speaker (Blind Mount) - White,1.118489583333,4.000000000000,Ø 11.57"" (294mm),7 locations  -     0.75/0.87/1.10"" (19/22/28mm),12,Steel - Black Powder coated,0,Ø 12.75"" (323.9mm),0
FC-8TPI - White,13.2,https://www.atlasied.com,"Laminate, White, Matte","30W, 15W, 7.5W, 3.8W ( 1.9W 70V) & Low Z operation","LF: (8"") 200mm Bass/Mid, mineral loaded polypropylene, HF: 1"" (25mm) titanium dome with neodymium magnet system, Ferrofluid cooled",0.677083333333,91dB,0,52,16.2"" x 37.4"" x 22.1"" (41cm x 95cm x 56cm),91,"UL1480A, UL2043, CE",1,160W @ 8 Ohms,109dB,110/116 dB,0.840533,https://www.atlasied.com/fc-8tpi,,160W,320W,80W,10,2,"Round black grill, square white grill, square black grill",-40°F to 140°F (-40° C to 60° C),8 Ohms,90°,FC-8TPI,9.000000000000,7.5,0,AtlasIED,6,Removable locking dinkle connector with screw terminals & loop through facility,"C-Ring, tile-bridge kit, cut-out template, round white grille",1,1,"Steel, weather resistent coating (Black)",Ø13.07"" (332mm),Grille Scrim - White,White Grille,13.42"" (341mm),12.63"" (321mm),77Hz-19kHz,58Hz-20kHz,1,0,0,0,0,0,Salt Spray & Chlorine,IP33,"Backcan: Powder Coated Steel (Black), Baffle: High Impact ABS UL-V0 (White), Grille: Steel, weather resistent coating (White)",12.000000000000,0,90,7.5,75,8"" Premium Ceiling Speaker (Pre-Install) - White,1.118489583333,4.000000000000,Ø 11.57"" (294mm),7 locations  -     0.75/0.87/1.10"" (19/22/28mm),12,Steel - Black Powder coated,0,Ø 12.75"" (323.9mm),0
FC-8ST,18.3,https://www.atlasied.com,"Laminate, White, Matte","30W, 15W, 7.5W, 3.8W ( 1.9W 70V) & Low Z operation","LF: (8"") 200mm Bass/Mid, mineral loaded polypropylene, HF: 1"" (25mm) titanium dome with neodymium magnet system, Ferrofluid cooled",0.677083333333,92dB,0,28.9,16.2"" x 28"" x 20.1"" (41cm x 71cm x 51cm),92,"UL1480A, UL2043, CE",1,200W @ 8 Ohms,110dB,111/118 dB,0.667659,https://www.atlasied.com/fc-8st,,200W,400W,100W,10,1,"Round black grill, square white grill, square black grill",-40°F to 140°F (-40° C to 60° C),8 Ohms,180°,FC-8ST,12.853332060679,7.5,0,AtlasIED,6,Removable locking dinkle connector with screw terminals & loop through facility,"C-Ring, tile-bridge kit, cut-out template, round white grille",1,1,"Steel, weather resistent coating (Black)",Ø13.07"" (332mm),Grille Scrim - White,White Grille,13.42"" (341mm),12.63"" (321mm),47Hz-140Hz,40Hz-200Hz,0,1,0,0,0,0,Salt Spray & Chlorine,IP33,"Backcan: Powder Coated Steel (Black), Baffle: High Impact ABS UL-V0 (White), Grille: Steel, weather resistent coating (White)",17.137776080905,0,110,,75,8"" Premium Ceiling Subwoofer (Blind Mount) - White,1.118489583333,4.000000000000,Ø 11.57"" (294mm),7 locations  -     0.75/0.87/1.10"" (19/22/28mm),12,Steel - Black Powder coated,0,Ø 12.75"" (323.9mm),0
