,Width##LENGTH##FEET,Weight Product##OTHER##,Vertical Steering##OTHER##,Vertical Opening Angle##OTHER##,URL##OTHER##,Typical Throw##OTHER##,Transducers (LF/HF)##OTHER##,System Sensitivity  (1W @ 1m)##OTHER##,Show AVIXA Symbol##OTHER##,Secondary Technology##OTHER##,Rotation Offset##ANGLE##DEGREES,Product Page URL##OTHER##,Product Documentation Link##OTHER##,Primary Technology##OTHER##,Power Supply##OTHER##,Mounting Type##OTHER##,Module Height##LENGTH##FEET,Model##OTHER##,Manufacturer##OTHER##,Low Frequency Beam Control Limit##OTHER##,Logo##OTHER##,Legend or Schedule Reference##OTHER##,Height##LENGTH##FEET,Hardware Finish##OTHER##,Grill Scrim##OTHER##,Grill Finish##OTHER##,Frequency Response (+/- 3dB)##OTHER##,External Control##OTHER##,Environmental##OTHER##,Enclosure##OTHER##,Dispersion Horizontal##OTHER##,Description##OTHER##,Depth##LENGTH##FEET,Default Elevation##LENGTH##FEET,DSP Function##OTHER##,DSP##OTHER##,Control##OTHER##,Configuration##OTHER##,Color##OTHER##,Case Finish##OTHER##,Bracket Spacing##LENGTH##FEET,Beam Steering##OTHER##,Azimuth##ANGLE##DEGREES,Audio Inputs##OTHER##,Amplifier##OTHER##,ALX 8##OTHER##,ALX 48##OTHER##,ALX 40##OTHER##,ALX 32##OTHER##,ALX 24##OTHER##,ALX 16##OTHER##,1/8 Full Power Watts##OTHER##
ALX-16D-W,0.391601562500,44,+40° to -40° (digitally variable),5° - 40° (digitally variable),atlasied.com,130ft / 40m,"16 x 4"" Neodymium, full range. Coated NRSC fiberglass membrane","15dBu RMS for rated output, analog",1,SA16,90.000000000000,https://www.atlasied.com/alx-16d,https://www.atlasied.com/ATS007619-ALX-16D-Data-Sheet_RevB.pdf,S,94 – 264V,W,2.664062500000,ALX-16D,Atlas IED,400Hz,"Laminate, White, Matte",,5.282226562500,Steel - White Powder coated,Grille Scrim - White,White Grille,"60Hz – 18kHz, 100dB @ 30 m","UDP commands, 2 x GPIO",IP64 (optional),Aluminum (powder coated),120° (- 6dB @ 1kHz – 8kHz),"Digitally Steerable, Multichannel 16-Speaker Column Array Loudspeaker",0.491536458333,4.000000000000,"24 presets switchable via GPIO UDP, 10 Band IIR Filter, FIR Filter, dynamic EQ, limiter, gain, 

delay, status display surveillance, automatically cascading",96kHz / 24 bit 1.8ms latency,"IP-based network, configurable",Full Range,"RAL 9016 standard (white)

all RAL colors available as an option",Steel - White Powder coated,5.355468750000,Multi beam,0.000000000000,2 x Dante® / AES67 / 2 x analog line / 2 x AES / EBU,16 x PWM class-D   16 x DSP Channels,1,0,0,0,0,1,63
ALX-4D-W,0.391601562500,12,+40° to -40° (digitally variable),5° - 40° (digitally variable),atlasied.com,30ft / 10m,"4 x 4"" Neodymium, full range. Coated NRSC fiberglass membrane","15dBu RMS for rated output, analog",1,SA16,90.000000000000,https://www.atlasied.com/alx-4d,https://www.atlasied.com/vcd/ATS007617-ALX-4D-Data-Sheet_RevB.pdf,S,94 – 264V,W,1.351562500000,ALX-4D-W,Atlas IED,1kHz,"Laminate, White, Matte",,1.351562500000,Steel - White Powder coated,Grille Scrim - White,White Grille,"100Hz - 18kHz, 94dB @ 30m","UDP commands, 2 x GPIO",IP64 (optional),Aluminum (powder coated),120° (- 6dB @ 1kHz – 8kHz),"Digitally Steerable, Multichannel 4-Speaker Column Array Loudspeaker",0.491536458333,4.000000000000,"24 presets switchable via GPIO UDP, 10 Band IIR Filter, FIR Filter, dynamic EQ, limiter, gain, 

delay, status display surveillance, automatically cascading",96kHz / 24 bit 1.8ms latency,"IP-based network, configurable",Full Range,"RAL 9016 standard (white)

all RAL colors available as an option",Steel - White Powder coated,1.390950520833,Multi beam,0.000000000000,2 x Dante® / AES67 / 2 x analog line / 2 x AES / EBU,4 x PWM class-D   4 x DSP Channels,0,0,0,0,0,0,63
ALX-4D-B,0.391601562500,12,+40° to -40° (digitally variable),5° - 40° (digitally variable),atlasied.com,30ft / 10m,"4 x 4"" Neodymium, full range. Coated NRSC fiberglass membrane","15dBu RMS for rated output, analog",1,SA16,90.000000000000,https://www.atlasied.com/alx-4d,https://www.atlasied.com/vcd/ATS007617-ALX-4D-Data-Sheet_RevB.pdf,S,94 – 264V,W,1.351562500000,ALX-4D-B,Atlas IED,1kHz,"Laminate, Black, Matte",,1.351562500000,Steel - Black Powder coated,Grille Scrim - Black,Black Grille,"100Hz - 18kHz, 94dB @ 30m","UDP commands, 2 x GPIO",IP64 (optional),Aluminum (powder coated),120° (- 6dB @ 1kHz – 8kHz),"Digitally Steerable, Multichannel 4-Speaker Column Array Loudspeaker",0.491536458333,4.000000000000,"24 presets switchable via GPIO UDP, 10 Band IIR Filter, FIR Filter, dynamic EQ, limiter, gain, 

delay, status display surveillance, automatically cascading",96kHz / 24 bit 1.8ms latency,"IP-based network, configurable",Full Range,Black,Steel - Black Powder coated,1.390950520833,Multi beam,0.000000000000,2 x Dante® / AES67 / 2 x analog line / 2 x AES / EBU,4 x PWM class-D   4 x DSP Channels,0,0,0,0,0,0,63
ALX-8D-B,0.391601562500,12,+40° to -40° (digitally variable),5° - 40° (digitally variable),atlasied.com,65ft / 20m,"8 x 4"" Neodymium, full range. Coated NRSC fiberglass membrane","15dBu RMS for rated output, analog",1,SA16,90.000000000000,https://www.atlasied.com/alx-8d,https://www.atlasied.com/vcd/ATS007618-ALX-8D-Data-Sheet_RevB.pdf,S,94 – 264V,W,2.664062500000,ALX-8D-B,Atlas IED,800Hz,"Laminate, Black, Matte",,2.664062500000,Steel - Black Powder coated,Grille Scrim - Black,Black Grille,"100Hz - 18kHz, 94dB @ 30m","UDP commands, 2 x GPIO",IP64 (optional),Aluminum (powder coated),120° (- 6dB @ 1kHz – 8kHz),"Digitally Steerable, Multichannel 8-Speaker Column Array Loudspeaker",0.491536458333,4.000000000000,"24 presets switchable via GPIO UDP, 10 Band IIR Filter, FIR Filter, dynamic EQ, limiter, gain, 

delay, status display surveillance, automatically cascading",96kHz / 24 bit 1.8ms latency,"IP-based network, configurable",Full Range,Black,Steel - Black Powder coated,2.708333333333,Multi beam,0.000000000000,2 x Dante® / AES67 / 2 x analog line / 2 x AES / EBU,8 x PWM class-D   8 x DSP Channels,1,0,0,0,0,0,63
ALX-8D-W,0.391601562500,12,+40° to -40° (digitally variable),5° - 40° (digitally variable),atlasied.com,65ft / 20m,"8 x 4"" Neodymium, full range. Coated NRSC fiberglass membrane","15dBu RMS for rated output, analog",1,SA16,90.000000000000,https://www.atlasied.com/alx-8d,https://www.atlasied.com/vcd/ATS007618-ALX-8D-Data-Sheet_RevB.pdf,S,94 – 264V,W,2.664062500000,ALX-8D-W,Atlas IED,800Hz,"Laminate, White, Matte",,2.664062500000,Steel - White Powder coated,Grille Scrim - White,White Grille,"100Hz - 18kHz, 94dB @ 30m","UDP commands, 2 x GPIO",IP64 (optional),Aluminum (powder coated),120° (- 6dB @ 1kHz – 8kHz),"Digitally Steerable, Multichannel 8-Speaker Column Array Loudspeaker",0.491536458333,4.000000000000,"24 presets switchable via GPIO UDP, 10 Band IIR Filter, FIR Filter, dynamic EQ, limiter, gain, 

delay, status display surveillance, automatically cascading",96kHz / 24 bit 1.8ms latency,"IP-based network, configurable",Full Range,Black,Steel - White Powder coated,2.708333333333,Multi beam,0.000000000000,2 x Dante® / AES67 / 2 x analog line / 2 x AES / EBU,8 x PWM class-D   8 x DSP Channels,1,0,0,0,0,0,63
ALX-16D-B,0.391601562500,44,+40° to -40° (digitally variable),5° - 40° (digitally variable),atlasied.com,130ft / 40m,"16 x 4"" Neodymium, full range. Coated NRSC fiberglass membrane","15dBu RMS for rated output, analog",1,SA16,90.000000000000,https://www.atlasied.com/alx-16d,https://www.atlasied.com/ATS007619-ALX-16D-Data-Sheet_RevB.pdf,S,94 – 264V,W,2.664062500000,ALX-16D,Atlas IED,400Hz,"Laminate, Black, Matte",,5.282226562500,Steel - Black Powder coated,Grille Scrim - Black,Black Grille,"60Hz – 18kHz, 100dB @ 30 m","UDP commands, 2 x GPIO",IP64 (optional),Aluminum (powder coated),120° (- 6dB @ 1kHz – 8kHz),"Digitally Steerable, Multichannel 16-Speaker Column Array Loudspeaker",0.491536458333,4.000000000000,"24 presets switchable via GPIO UDP, 10 Band IIR Filter, FIR Filter, dynamic EQ, limiter, gain, 

delay, status display surveillance, automatically cascading",96kHz / 24 bit 1.8ms latency,"IP-based network, configurable",Full Range,"RAL 9016 standard (white)

all RAL colors available as an option",Steel - Black Powder coated,5.355468750000,Multi beam,0.000000000000,2 x Dante® / AES67 / 2 x analog line / 2 x AES / EBU,16 x PWM class-D   16 x DSP Channels,1,0,0,0,0,1,63
ALX-24D-B,0.391601562500,44,+40° to -40° (digitally variable),5° - 40° (digitally variable),atlasied.com,190ft / 60m,"24 x 4"" Neodymium, full range. Coated NRSC fiberglass membrane","15dBu RMS for rated output, analog",1,SA16,90.000000000000,https://www.atlasied.com/alx-24d,https://www.atlasied.com/vcd/ATS007620-ALX-24D-Data-Sheet_RevB.pdf,S,94 – 264V,W,2.664062500000,ALX-24D-B,Atlas IED,250Hz,"Laminate, Black, Matte",,7.992187500000,Steel - Black Powder coated,Grille Scrim - Black,Black Grille,"60Hz - 18kHz, 103dB @ 30m","UDP commands, 2 x GPIO",IP64 (optional),Aluminum (powder coated),120° (- 6dB @ 1kHz – 8kHz),"Digitally Steerable, Multichannel 24-Speaker Column Array Loudspeaker",0.491536458333,4.000000000000,"24 presets switchable via GPIO UDP, 10 Band IIR Filter, FIR Filter, dynamic EQ, limiter, gain, 

delay, status display surveillance, automatically cascading",96kHz / 24 bit 1.8ms latency,"IP-based network, configurable",Full Range,"RAL 9016 standard (white)

all RAL colors available as an option",Steel - Black Powder coated,8.018229166667,Multi beam,0.000000000000,2 x Dante® / AES67 / 2 x analog line / 2 x AES / EBU,24 x PWM class-D   24 x DSP Channels,1,0,0,0,1,1,63
ALX-24D-W,0.391601562500,44,+40° to -40° (digitally variable),5° - 40° (digitally variable),atlasied.com,190ft / 60m,"24 x 4"" Neodymium, full range. Coated NRSC fiberglass membrane","15dBu RMS for rated output, analog",1,SA16,90.000000000000,https://www.atlasied.com/alx-24d,https://www.atlasied.com/vcd/ATS007620-ALX-24D-Data-Sheet_RevB.pdf,S,94 – 264V,W,2.664062500000,ALX-24D-W,Atlas IED,250Hz,"Laminate, White, Matte",,7.992187500000,Steel - White Powder coated,Grille Scrim - White,White Grille,"60Hz - 18kHz, 103dB @ 30m","UDP commands, 2 x GPIO",IP64 (optional),Aluminum (powder coated),120° (- 6dB @ 1kHz – 8kHz),"Digitally Steerable, Multichannel 24-Speaker Column Array Loudspeaker",0.491536458333,4.000000000000,"24 presets switchable via GPIO UDP, 10 Band IIR Filter, FIR Filter, dynamic EQ, limiter, gain, 

delay, status display surveillance, automatically cascading",96kHz / 24 bit 1.8ms latency,"IP-based network, configurable",Full Range,"RAL 9016 standard (white)

all RAL colors available as an option",Steel - White Powder coated,8.018229166667,Multi beam,0.000000000000,2 x Dante® / AES67 / 2 x analog line / 2 x AES / EBU,24 x PWM class-D   24 x DSP Channels,1,0,0,0,1,1,63
ALX-32D-W,0.391601562500,88,+40° to -40° (digitally variable),5° - 40° (digitally variable),atlasied.com,200ft / 80m,"32 x 4"" Neodymium, full range. Coated NRSC fiberglass membrane","15dBu RMS for rated output, analog",1,SA16,90.000000000000,https://www.atlasied.com/alx-32d,https://www.atlasied.com/vcd/ATS007620-ALX-32D-Data-Sheet_RevB.pdf,S,94 – 264V,W,2.664062500000,ALX-32D-W,Atlas IED,250Hz,"Laminate, White, Matte",,10.656250000000,Steel - White Powder coated,Grille Scrim - White,White Grille,"60Hz - 18kHz, 103dB @ 30m","UDP commands, 2 x GPIO",IP64 (optional),Aluminum (powder coated),120° (- 6dB @ 1kHz – 8kHz),"Digitally Steerable, Multichannel 32-Speaker Column Array Loudspeaker",0.491536458333,4.000000000000,"24 presets switchable via GPIO UDP, 10 Band IIR Filter, FIR Filter, dynamic EQ, limiter, gain, 

delay, status display surveillance, automatically cascading",96kHz / 24 bit 1.8ms latency,"IP-based network, configurable",Full Range,"RAL 9016 standard (white)

all RAL colors available as an option",Steel - White Powder coated,10.682291666667,Multi beam,0.000000000000,2 x Dante® / AES67 / 2 x analog line / 2 x AES / EBU,32 x PWM class-D   32 x DSP Channels,1,0,0,1,1,1,63
ALX-32D-B,0.391601562500,88,+40° to -40° (digitally variable),5° - 40° (digitally variable),atlasied.com,270ft / 80m,"32 x 4"" Neodymium, full range. Coated NRSC fiberglass membrane","15dBu RMS for rated output, analog",1,SA16,90.000000000000,https://www.atlasied.com/alx-32d,https://www.atlasied.com/vcd/ATS007621-ALX-32D-Data-Sheet_RevB.pdf,S,94 – 264V,W,2.664062500000,ALX-32D-B,Atlas IED,150Hz,"Laminate, Black, Matte",,13.320312500000,Steel - Black Powder coated,Grille Scrim - Black,Black Grille,"60Hz - 18kHz, 110dB @ 30m","UDP commands, 2 x GPIO",IP64 (optional),Aluminum (powder coated),120° (- 6dB @ 1kHz – 8kHz),"Digitally Steerable, Multichannel 32-Speaker Column Array Loudspeaker",0.491536458333,4.000000000000,"24 presets switchable via GPIO UDP, 10 Band IIR Filter, FIR Filter, dynamic EQ, limiter, gain, 

delay, status display surveillance, automatically cascading",96kHz / 24 bit 1.8ms latency,"IP-based network, configurable",Full Range,"RAL 9016 standard (white)

all RAL colors available as an option",Steel - Black Powder coated,10.682291666667,Multi beam,0.000000000000,2 x Dante® / AES67 / 2 x analog line / 2 x AES / EBU,32 x PWM class-D   32 x DSP Channels,1,0,0,1,1,1,63
ALX-40D-B,0.391601562500,110,+40° to -40° (digitally variable),5° - 40° (digitally variable),atlasied.com,295ft / 90m,"40 x 4"" Neodymium, full range. Coated NRSC fiberglass membrane","15dBu RMS for rated output, analog",1,SA16,90.000000000000,https://www.atlasied.com/alx-40d,https://www.atlasied.com/vcd/ATS007620-ALX-40D-Data-Sheet_RevB.pdf,S,94 – 264V,W,2.664062500000,ALX-40D-B,Atlas IED,150Hz,"Laminate, Black, Matte",,13.320312500000,Steel - Black Powder coated,Grille Scrim - Black,Black Grille,"60Hz - 18kHz, 110dB @ 30m","UDP commands, 2 x GPIO",IP64 (optional),Aluminum (powder coated),120° (- 6dB @ 1kHz – 8kHz),"Digitally Steerable, Multichannel 40-Speaker Column Array Loudspeaker",0.491536458333,4.000000000000,"24 presets switchable via GPIO UDP, 10 Band IIR Filter, FIR Filter, dynamic EQ, limiter, gain, 

delay, status display surveillance, automatically cascading",96kHz / 24 bit 1.8ms latency,"IP-based network, configurable",Full Range,"RAL 9016 standard (white)

all RAL colors available as an option",Steel - Black Powder coated,13.346354166667,Multi beam,0.000000000000,2 x Dante® / AES67 / 2 x analog line / 2 x AES / EBU,40 x PWM class-D   40 x DSP Channels,1,0,1,1,1,1,63
ALX-40D-W,0.391601562500,110,+40° to -40° (digitally variable),5° - 40° (digitally variable),atlasied.com,295ft / 90m,"40 x 4"" Neodymium, full range. Coated NRSC fiberglass membrane","15dBu RMS for rated output, analog",1,SA16,90.000000000000,https://www.atlasied.com/alx-40d,https://www.atlasied.com/vcd/ATS007620-ALX-40D-Data-Sheet_RevB.pdf,S,94 – 264V,W,2.664062500000,ALX-40D-W,Atlas IED,150Hz,"Laminate, White, Matte",,13.320312500000,Steel - White Powder coated,Grille Scrim - White,White Grille,"60Hz - 18kHz, 110dB @ 30m","UDP commands, 2 x GPIO",IP64 (optional),Aluminum (powder coated),120° (- 6dB @ 1kHz – 8kHz),"Digitally Steerable, Multichannel 40-Speaker Column Array Loudspeaker",0.491536458333,4.000000000000,"24 presets switchable via GPIO UDP, 10 Band IIR Filter, FIR Filter, dynamic EQ, limiter, gain, 

delay, status display surveillance, automatically cascading",96kHz / 24 bit 1.8ms latency,"IP-based network, configurable",Full Range,"RAL 9016 standard (white)

all RAL colors available as an option",Steel - White Powder coated,13.346354166667,Multi beam,0.000000000000,2 x Dante® / AES67 / 2 x analog line / 2 x AES / EBU,40 x PWM class-D   40 x DSP Channels,1,0,1,1,1,1,63
ALX-48D-W,0.391601562500,132,+40° to -40° (digitally variable),5° - 40° (digitally variable),atlasied.com,325ft / 100m,"48 x 4"" Neodymium, full range. Coated NRSC fiberglass membrane","15dBu RMS for rated output, analog",1,SA16,90.000000000000,https://www.atlasied.com/alx-48d,https://www.atlasied.com/vcd/ATS007623-ALX-48D-Data-Sheet_RevC.pdf,S,94 – 264V,W,2.664062500000,ALX-48D-W,Atlas IED,90Hz,"Laminate, White, Matte",,15.984375000000,Steel - White Powder coated,Grille Scrim - White,White Grille,"60Hz - 18kHz, 110dB @ 30m","UDP commands, 2 x GPIO",IP64 (optional),Aluminum (powder coated),120° (- 6dB @ 1kHz – 8kHz),"Digitally Steerable, Multichannel 48-Speaker Column Array Loudspeaker",0.491536458333,4.000000000000,"24 presets switchable via GPIO UDP, 10 Band IIR Filter, FIR Filter, dynamic EQ, limiter, gain, 

delay, status display surveillance, automatically cascading",96kHz / 24 bit 1.8ms latency,"IP-based network, configurable",Full Range,"RAL 9016 standard (white)

all RAL colors available as an option",Steel - White Powder coated,16.005208333333,Multi beam,0.000000000000,2 x Dante® / AES67 / 2 x analog line / 2 x AES / EBU,48 x PWM class-D   48 x DSP Channels,1,1,1,1,1,1,63
ALX-48D-B,0.391601562500,132,+40° to -40° (digitally variable),5° - 40° (digitally variable),atlasied.com,325ft / 100m,"48 x 4"" Neodymium, full range. Coated NRSC fiberglass membrane","15dBu RMS for rated output, analog",1,SA16,90.000000000000,https://www.atlasied.com/alx-48d,https://www.atlasied.com/vcd/ATS007623-ALX-48D-Data-Sheet_RevC.pdf,S,94 – 264V,W,2.664062500000,ALX-48D-B,Atlas IED,90Hz,"Laminate, Black, Matte",,15.984375000000,Steel - Black Powder coated,Grille Scrim - Black,Black Grille,"60Hz - 18kHz, 110dB @ 30m","UDP commands, 2 x GPIO",IP64 (optional),Aluminum (powder coated),120° (- 6dB @ 1kHz – 8kHz),"Digitally Steerable, Multichannel 48-Speaker Column Array Loudspeaker",0.491536458333,4.000000000000,"24 presets switchable via GPIO UDP, 10 Band IIR Filter, FIR Filter, dynamic EQ, limiter, gain, 

delay, status display surveillance, automatically cascading",96kHz / 24 bit 1.8ms latency,"IP-based network, configurable",Full Range,"RAL 9016 standard (white)

all RAL colors available as an option",Steel - Black Powder coated,16.005208333333,Multi beam,0.000000000000,2 x Dante® / AES67 / 2 x analog line / 2 x AES / EBU,48 x PWM class-D   48 x DSP Channels,1,1,1,1,1,1,63
