,Weight (lbs)##OTHER##,Wallboard Thickness##LENGTH##INCHES,URL##OTHER##,Speaker Material##OTHER##,Model##OTHER##,Max SPL##OTHER##,Manufacturer##OTHER##,Ingress Protection##OTHER##,IP-STBE##OTHER##,IP-STB##OTHER##,IP-SEST-S##OTHER##,IP-SEA-S##OTHER##,IP-FEST-S##OTHER##,Frequency Range##OTHER##,Enclosure Material##OTHER##,Default Elevation##LENGTH##INCHES,Coverage##ANGLE##DEGREES,Ceiling Tile Thickness##LENGTH##INCHES
IP-8SM + IP-FEST-S enclosure,3.6,0.5,www.atlasied.com,Aluminum - White,IP-8SM,120,AtlasIED,IP-30,0,0,0,0,1,86Hz - 15.5kHz,Steel - White,48,105.000000000000,0.5
IP-8SM + IP-SEA-S enclosure,3.6,0.5,www.atlasied.com,Aluminum - White,IP-8SM,120,AtlasIED,IP-30,0,0,0,1,0,86Hz - 15.5kHz,Steel - White,48,105.000000000000,0.5
IP-8SM + IP-SEST-S enclosure,3.6,0.5,www.atlasied.com,Aluminum - White,IP-8SM,120,AtlasIED,IP-30,0,1,0,0,0,86Hz - 15.5kHz,Steel - White,48,105.000000000000,0.5
IP-8SM + IP-STB tile bridge,3.6,0.5,www.atlasied.com,Aluminum - White,IP-8SM,120,AtlasIED,IP-30,1,0,0,0,0,86Hz - 15.5kHz,Steel - White,48,105.000000000000,0.5
IP-8SM + IP-STBE tile bridge enclosure,3.6,0.5,www.atlasied.com,Aluminum - White,IP-8SM,120,AtlasIED,IP-30,0,0,1,0,0,86Hz - 15.5kHz,Steel - White,48,105.000000000000,0.5
