,base offset##LENGTH##INCHES,Weight (lbs)##OTHER##,Wallboard Thickness##LENGTH##INCHES,URL##OTHER##,Speaker Material##OTHER##,Model##OTHER##,Max SPL##OTHER##,Manufacturer##OTHER##,IP-SEST-HVP##OTHER##,IP-FEST-HVP##OTHER##,Frequency Response##OTHER##,Enclosure Material##OTHER##,Default Elevation##LENGTH##INCHES,Coverage Cone##OTHER##,Coverage##ANGLE##DEGREES
IP-HVP + IP-FEST-HVP enclosure,0.15,5.11,0.5,,Aluminum - White,,120,,0,1,600Hz - 14kHz,Steel - White,48,0,95.000000000000
IP-HVP + IP-SEST-HVP enclosure,6.15,5.11,0.5,www.atlasied.com,Aluminum - White,IP-HVP,120,AtlasIED,1,0,600Hz - 14kHz,Steel - White,48,0,95.000000000000
