,Weight (lbs)##OTHER##,Wallboard Thickness##LENGTH##INCHES,URL##OTHER##,Model##OTHER##,Max SPL##OTHER##,Manufacturer##OTHER##,IP-SEST-SD##OTHER##,IP-SEA-SD##OTHER##,IP-FEST-SD##OTHER##,Grille##OTHER##,Frequency Response##OTHER##,Flasher##OTHER##,Display##OTHER##,Default Elevation##LENGTH##INCHES,Coverage##ANGLE##DEGREES
IP-SDMF + IP-SEST-SD enclosure,4.25,0.5,www.atlasied.com,IP-SDMF,110,AtlasIED,1,0,0,1,86Hz - 15.5kHz (+/- 5dB),1,1,48,105.000000000000
IP-SDMF + IP-SEA-SD enclosure,4.25,0.5,www.atlasied.com,IP-SDMF,110,AtlasIED,0,1,0,1,86Hz - 15.5kHz (+/- 5dB),1,1,48,105.000000000000
IP-SDMF + IP-FEST-SD enclosure,4.25,0.5,www.atlasied.com,IP-SDMF,110,AtlasIED,0,0,1,1,86Hz - 15.5kHz (+/- 5dB),1,1,48,105.000000000000
IP-SDM + IP-SEST-SD enclosure,4.25,0.5,www.atlasied.com,IP-SDMF,110,AtlasIED,1,0,0,1,86Hz - 15.5kHz (+/- 5dB),0,1,48,105.000000000000
IP-SDM + IP-SEA-SD enclosure,4.25,0.5,www.atlasied.com,IP-SDMF,110,AtlasIED,0,1,0,1,86Hz - 15.5kHz (+/- 5dB),0,1,48,105.000000000000
IP-SDM + IP-FEST-SD enclosure,4.25,0.5,www.atlasied.com,IP-SDMF,110,AtlasIED,0,0,1,1,86Hz - 15.5kHz (+/- 5dB),0,1,48,105.000000000000
IP-SM + IP-SEST-SD enclosure,4.25,0.5,www.atlasied.com,IP-SDMF,110,AtlasIED,1,0,0,1,86Hz - 15.5kHz (+/- 5dB),0,0,48,105.000000000000
IP-SM + IP-SEA-SD enclosure,4.25,0.5,www.atlasied.com,IP-SDMF,110,AtlasIED,0,1,0,1,86Hz - 15.5kHz (+/- 5dB),0,0,48,105.000000000000
IP-SM + IP-FEST-SD enclosure,4.25,0.5,www.atlasied.com,IP-SDMF,110,AtlasIED,0,0,1,1,86Hz - 15.5kHz (+/- 5dB),0,0,48,105.000000000000
IP-SDH + IP-SEST-SD enclosure,5.21,0.5,www.atlasied.com,IP-SDMF,110,AtlasIED,1,0,0,1,600Hz - 14kHz (+/- 5dB),0,1,48,95.000000000000
IP-SDH + IP-SEA-SD enclosure,5.21,0.5,www.atlasied.com,IP-SDMF,110,AtlasIED,0,1,0,1,600Hz - 14kHz (+/- 5dB),0,1,48,95.000000000000
IP-SDH + IP-FEST-SD enclosure,5.21,0.5,www.atlasied.com,IP-SDMF,110,AtlasIED,0,0,1,1,600Hz - 14kHz (+/- 5dB),0,1,48,95.000000000000
