,Weight (lbs)##OTHER##,URL##OTHER##,Transformer Taps##OTHER##,Tile Bars##OTHER##,Speaker Type Visible##OTHER##,Speaker Type Annotation##OTHER##,Sensitivity##OTHER##,SPL Target##OTHER##,REP##OTHER##,Peak Factor##OTHER##,Mount Material##OTHER##,Model##OTHER##,Minimum Tap##OTHER##,Minimum Overlap Guide##OTHER##,Max SPL (Peak)##OTHER##,Manufacturer##OTHER##,Listener Height##LENGTH##INCHES,Ingress Protection##OTHER##,Grille Scrim Material##OTHER##,Grille Material##OTHER##,Grille##OTHER##,Frequency Response##OTHER##,Enclosure Material##OTHER##,Edge-To-Edge Guide##OTHER##,Doglegs Stowed##OTHER##,Dispersion Cone Visible##OTHER##,Dispersion Cone Height##LENGTH##INCHES,Dispersion##ANGLE##DEGREES,Description##OTHER##,Default Elevation##LENGTH##INCHES,Certifications##OTHER##,Ceiling Thickness##LENGTH##INCHES,Ceiling Height##LENGTH##INCHES,C-Ring##OTHER##,Baffle Material##OTHER##
FAP63TC-W,8.75,www.atlasied.com,"4W, 8W, 16W, 32W",1,0,S1,90,75,1.440285,10,Plastic - White - Smooth,FAP63TC-W,4,0,115,AtlasIED,5,IP-21,Grille Scrim - White,Grille - White,1,80Hz - 20kHz (+/- 5dB),Steel - Gray epoxy,0,0,0,7,130.000000000000,"Full Range, Shallow Mount, Ceiling Loudspeaker",48,"UL Listed to UL1480, UL2043 and CSA C22.2",0.5,12,1,Plastic - White - Smooth
