The FS-xT and FS-xD models utilize the same passive crossovers and transducers, therefore the same EASE GLL.
In EASE 5 & EASE Focus the attenuation adjustments to account for the type of POE power are shown in the tables below - 


FS-4D			EASE Attenuation	Power
POE++ (Type 4)		0dB			60W (DSP limited)
POE++ (Type 3)		0dB			60W
POE+ (Type 2)		-3dB			30W
		
		
FS-6D			EASE Attenuation	Power
POE++ (Type 4)		0dB	         	90W
POE++ (Type 3)		-1.7dB	         	60W
POE+ (Type 2)		-4.7dB	         	30W
