,Width##LENGTH##FEET,Weight Product##OTHER##,URL##OTHER##,Trim##OTHER##,Transducers (LF/HF)##OTHER##,Target SPL##OTHER##,PoE++ Type 4##OTHER##,PoE++ Type 3##OTHER##,PoE+ Type 2##OTHER##,System Sensitivity  (1W @ 1m)##OTHER##,Supported PoE standard(s)##OTHER##,Supported AoIP formats##OTHER##,Static IP supported##OTHER##,Sensitivity##OTHER##,Safety Agency Rating##OTHER##,Rotation Offset##ANGLE##DEGREES,Rotation##ANGLE##DEGREES,Remove Logo##OTHER##,REP##OTHER##,Product Page URL##OTHER##,Product Documentation Link##OTHER##,Power Output - Single Channel (W)##OTHER##,Power Output - Dual Channel (W)##OTHER##,Peak Factor##OTHER##,Optional Accessories##OTHER##,Operating Temperature##OTHER##,Nominal Coverage Angle  (HxV -6dB)##OTHER##,Model##OTHER##,Maximum SPL (Peak)##OTHER##,Maximum SPL (Average)##OTHER##,Manufacturer##OTHER##,Logo Constraint##OTHER##,Logo##OTHER##,Input Connector##OTHER##,Included Accessories##OTHER##,Height##LENGTH##FEET,Hardware Finish##OTHER##,Grille Material##OTHER##,Grill Scrim##OTHER##,Grill Finish##OTHER##,Frequency Response (+/- 3dB)##OTHER##,Frequency  Range (-10dB)##OTHER##,FS-6 Peak##OTHER##,FS-4 Peak##OTHER##,Environmental Testing##OTHER##,Environmental##OTHER##,Enclosure##OTHER##,Dispersion##ANGLE##DEGREES,Directivity Index (dB)##OTHER##,Description##OTHER##,Depth##LENGTH##FEET,Default Elevation##LENGTH##FEET,D2##LENGTH##FEET,Current Consumption at Idle (mA)##OTHER##,Current Consumption Peak (mA)##OTHER##,Case Finish 2##OTHER##,Case Finish##OTHER##,Azimuth Offset##ANGLE##DEGREES,Azimuth##ANGLE##DEGREES,FS-4##OTHER##,FS-6##OTHER##
FS-4D-B,0.573242187500,7.72,www.atlasied.com,"Laminate, Black, Matte","LF: 4"" (100mm)  Bass/Mid, mineral loaded polypropylene, HF: 0.75"" (19mm) titanium dome with neodymium magnet system, Ferrofluid cooled",75,1,0,0,87dB,PoE+ Type 2 / PoE++ Type 3 / PoE++ Type 4,"Dante, AES67",1,87,"Conforms to UL62368-1, Certified to CSA STD 22.2 No. 62368-1, EMC - FCC Part 15, Subpart B, EN 55032, EN 55035, EN IEC 6100, EN 6100",90.000000000000,0.000000000000,0,23.459897,,,90,45,10,Pan & Tilt Bracket (AS-U-B/AS-U-W),-40°F to 140°F (-40° C to 60° C),115° Conical,FS-4D-B,111,105,AtlasIED,1,"Laminate, Black, Matte",Euroblock with screw connections and loop output,Slip Free U-Bracket,0.908203125000,"Metal, Powder Coated, Black","Aluminium, Powder Coated",Grille Scrim - Black,Black Grille,83Hz-22kHz,63Hz-30kHz,114,111,Conforms to MIL-STD-810 for salt spray & humidity,IP65,High Impact ABS UL-V0,115.000000000000,6.1,"Two-Way, Full Range, POE, Surface Mount Loudspeaker - Black",0.672526041667,4.000000000000,20.000000000000,28,757,"Laminate, Black, Matte","Laminate, Black, Matte",90.000000000000,0.000000000000,1,0
FS-4D-W,0.573242187500,7.72,www.atlasied.com,"Laminate, White, Matte","LF: 4"" (100mm)  Bass/Mid, mineral loaded polypropylene, HF: 0.75"" (19mm) titanium dome with neodymium magnet system, Ferrofluid cooled",75,1,0,0,87dB,PoE+ Type 2 / PoE++ Type 3 / PoE++ Type 4,"Dante, AES67",1,87,"Conforms to UL62368-1, Certified to CSA STD 22.2 No. 62368-1, EMC - FCC Part 15, Subpart B, EN 55032, EN 55035, EN IEC 6100, EN 6100",90.000000000000,0.000000000000,0,23.459897,,,90,45,10,Pan & Tilt Bracket (AS-U-B/AS-U-W),-40°F to 140°F (-40° C to 60° C),115° Conical,FS-4D-W,111,105,AtlasIED,1,"Laminate, White, Matte",Euroblock with screw connections and loop output,Slip Free U-Bracket,0.908203125000,"Metal, Powder Coated, White","Aluminium, Powder Coated",Grille Scrim - White,White Grille,83Hz-22kHz,63Hz-30kHz,114,111,Conforms to MIL-STD-810 for salt spray & humidity,IP65,High Impact ABS UL-V0,115.000000000000,6.1,"Two-Way, Full Range, POE, Surface Mount Loudspeaker - Black",0.672526041667,4.000000000000,20.000000000000,28,757,"Laminate, White, Matte","Laminate, White, Matte",90.000000000000,0.000000000000,1,0
FS-6D-B,0.644205729167,12.02,www.atlasied.com,"Laminate, Black, Matte","LF: 6"" (150mm) Bass/Mid, mineral loaded polypropylene, HF: 1"" (25mm) titanium dome with neodymium magnet system, Ferrofluid cooled",75,1,0,0,89dB,PoE+ Type 2 / PoE++ Type 3 / PoE++ Type 4,"Dante, AES67",1,89,"Conforms to UL62368-1, Certified to CSA STD 22.2 No. 62368-1, EMC - FCC Part 15, Subpart B, EN 55032, EN 55035, EN IEC 6100, EN 6100",90.000000000000,0.000000000000,0,14.802194,,,90,45,10,Pan & Tilt Bracket (AS-UL-B/AS-UL-W),-40°F to 140°F (-40° C to 60° C),100° Conical,FS-6D-B,114,108,AtlasIED,1,"Laminate, Black, Matte",Euroblock with screw connections and loop output,Slip Free U-Bracket,1.158203125000,"Metal, Powder Coated, Black","Aluminium, Powder Coated",Grille Scrim - Black,Black Grille,72Hz-22kHz,57Hz-30kHz,114,111,Conforms to MIL-STD-810 for salt spray & humidity,IP65,High Impact ABS UL-V0,100.000000000000,8.2,"Two-Way, Full Range, POE, Surface Mount Loudspeaker - Black",0.721679687500,4.000000000000,20.000000000000,28,757,"Laminate, Black, Matte","Laminate, Black, Matte",90.000000000000,0.000000000000,0,1
FS-6D-W,0.644205729167,12.02,www.atlasied.com,"Laminate, White, Matte","LF: 6"" (150mm) Bass/Mid, mineral loaded polypropylene, HF: 1"" (25mm) titanium dome with neodymium magnet system, Ferrofluid cooled",75,1,0,0,89dB,PoE+ Type 2 / PoE++ Type 3 / PoE++ Type 4,"Dante, AES67",1,89,"Conforms to UL62368-1, Certified to CSA STD 22.2 No. 62368-1, EMC - FCC Part 15, Subpart B, EN 55032, EN 55035, EN IEC 6100, EN 6100",90.000000000000,0.000000000000,0,14.802194,,,90,45,10,Pan & Tilt Bracket (AS-UL-B/AS-UL-W),-40°F to 140°F (-40° C to 60° C),100° Conical,FS-6D-W,114,108,AtlasIED,1,"Laminate, White, Matte",Euroblock with screw connections and loop output,Slip Free U-Bracket,1.158203125000,"Metal, Powder Coated, White","Aluminium, Powder Coated",Grille Scrim - White,White Grille,72Hz-22kHz,57Hz-30kHz,114,111,Conforms to MIL-STD-810 for salt spray & humidity,IP65,High Impact ABS UL-V0,100.000000000000,8.2,"Two-Way, Full Range, POE, Surface Mount Loudspeaker - Black",0.721679687500,4.000000000000,20.000000000000,28,757,"Laminate, White, Matte","Laminate, White, Matte",90.000000000000,0.000000000000,0,1
