,Weight Product##OTHER##,URL##OTHER##,Trim##OTHER##,Transducers (LF/HF)##OTHER##,Tile Bridge Spacing##LENGTH##INCHES,Supported PoE Standards##OTHER##,Supported AoIP formats##OTHER##,Static IP supported##OTHER##,Square Grille##OTHER##,Shipping Dimensions (HxWxD)##OTHER##,Sensitivity##OTHER##,Safety Agency Rating##OTHER##,SPL Target##OTHER##,Round Grille##OTHER##,REP##OTHER##,Product Page URL##OTHER##,Product Documentation Link##OTHER##,Power Output - Single Channel (W)##OTHER##,Power Output - Dual Channel (W)##OTHER##,PoE++ Type 4##OTHER##,PoE++ Type 3##OTHER##,Peak Factor##OTHER##,Packed Qty##OTHER##,PoE+ Type 2##OTHER##,Optional Accessories##OTHER##,Operating Temperature##OTHER##,Model##OTHER##,Minimum Overlap Spacing##LENGTH##INCHES,Min Overlap Guide##OTHER##,Maximum SPL (Peak)##OTHER##,Maximum SPL (Average)##OTHER##,Manufacturer##OTHER##,Listener Height##OTHER##,Input Connector##OTHER##,Included Accessories##OTHER##,Include Tile Bridge##OTHER##,Include C Ring##OTHER##,Grille Material##OTHER##,Grille Diameter##OTHER##,Grill Scrim##OTHER##,Grill Finish##OTHER##,Front of ceiling to top of safety loop##OTHER##,Front of ceiling to rear of backcan##OTHER##,Frequency Response (+/- 3dB)##OTHER##,Frequency  Range (-10dB)##OTHER##,FC 8 Peak##OTHER##,FC 6 Peak##OTHER##,FC 4 Peak##OTHER##,FC-8##OTHER##,FC-6##OTHER##,FC-4##OTHER##,Environmental Testing##OTHER##,Environmental##OTHER##,Enclosure##OTHER##,Edge-To-Edge Spacing##LENGTH##INCHES,Edge-To-Edge Guide##OTHER##,Dispersion##ANGLE##DEGREES,Directivity Index (dB)##OTHER##,Description##OTHER##,Depth##LENGTH##INCHES,Default Elevation##LENGTH##INCHES,Cutout Diameter##OTHER##,Current Consumption at Idle (mA)##OTHER##,Current Consumption Peak (mA)##OTHER##,Ceiling Height##OTHER##,Case Finish##OTHER##,Black Round Grille##OTHER##,Bezel Diameter##OTHER##
FC-8D - Black,13.2,https://www.atlasied.com,"Laminate, Black","LF: (8"") 200mm Bass/Mid, mineral loaded polypropylene, HF: 1"" (25mm) titanium dome with neodymium magnet system, Ferrofluid cooled",8.125,PoE+ Type 2 / PoE++ Type 3 / PoE++ Type 4,"Dante, AES67",1,0,16.2"" x 37.4"" x 22.1"" (41cm x 95cm x 56cm),92,"UL2043, Conforms to UL62368-1, Certified to CSA STD 22.2 No. 62368-1                    EMC- FCC Part 15, Subpart B, EN 55032, EN 55035, EN IEC 6100, EN 6100",75,1,0.667659,https://www.atlasied.com/,,90,45,1,0,10,2,0,"Round black grill, square white grill, square black grill",-40°F to 140°F (-40° C to 60° C),FC-8D,108,0,118,112,AtlasIED,6,Removable locking dinkle connector with screw terminals & loop through facility,"C-Ring, tile-bridge kit, cut-out template, round white grille",1,1,"Steel, weather resistent coating (Black)",Ø13.07"" (332mm),Grille Scrim - Black,Black Grille,13.42"" (341mm),12.63"" (321mm),59Hz-25kHz,44Hz-30kHz,118,116,112,1,0,0,Salt Spray & Chlorine,IP33,"Backcan: Powder Coated Steel (Black), Baffle: High Impact ABS UL-V0 (White), Grille: Steel, weather resistent coating (White)",144,0,90.000000000000,7.5,8"" Premium POE Ceiling Speaker (Blind Mount) - White,13.421875,48,Ø 11.57"" (294mm),28,757,12,Steel - Black Powder coated,0,Ø 12.75"" (323.9mm)
FC-8D - White,13.2,https://www.atlasied.com,"Laminate, White, Matte","LF: (8"") 200mm Bass/Mid, mineral loaded polypropylene, HF: 1"" (25mm) titanium dome with neodymium magnet system, Ferrofluid cooled",8.125,PoE+ Type 2 / PoE++ Type 3 / PoE++ Type 4,"Dante, AES67",1,0,16.2"" x 37.4"" x 22.1"" (41cm x 95cm x 56cm),92,"UL2043, Conforms to UL62368-1, Certified to CSA STD 22.2 No. 62368-1                    EMC- FCC Part 15, Subpart B, EN 55032, EN 55035, EN IEC 6100, EN 6100",75,1,0.667659,https://www.atlasied.com/,,90,45,1,0,10,2,0,"Round black grill, square white grill, square black grill",-40°F to 140°F (-40° C to 60° C),FC-8D,108,0,118,112,AtlasIED,6,Removable locking dinkle connector with screw terminals & loop through facility,"C-Ring, tile-bridge kit, cut-out template, round white grille",1,1,"Steel, weather resistent coating (Black)",Ø13.07"" (332mm),Grille Scrim - White,White Grille,13.42"" (341mm),12.63"" (321mm),59Hz-25kHz,44Hz-30kHz,118,116,112,1,0,0,Salt Spray & Chlorine,IP33,"Backcan: Powder Coated Steel (Black), Baffle: High Impact ABS UL-V0 (White), Grille: Steel, weather resistent coating (White)",144,0,90.000000000000,7.5,8"" Premium POE Ceiling Speaker (Blind Mount) - White,13.421875,48,Ø 11.57"" (294mm),28,757,12,Steel - Black Powder coated,0,Ø 12.75"" (323.9mm)
FC-6D - Black,13.2,https://www.atlasied.com,"Laminate, Black","LF: (6"") 150mm Bass/Mid, mineral loaded polypropylene, HF: 1"" (25mm) titanium dome with neodymium magnet system, Ferrofluid cooled",7.125,PoE+ Type 2 / PoE++ Type 3 / PoE++ Type 4,"Dante, AES67",1,0,14.6"" x 33.7"" x 18.1"" (37cm x 85.5cm x 46cm),91,"UL2043, Conforms to UL62368-1, Certified to CSA STD 22.2 No. 62368-1                    EMC- FCC Part 15, Subpart B, EN 55032, EN 55035, EN IEC 6100, EN 6100",75,1,1.144059,https://www.atlasied.com/,,90,45,1,0,10,2,0,"Round black grill, square white grill, square black grill",-40°F to 140°F (-40° C to 60° C),FC-6D,150.16095266687,0,116,110,AtlasIED,5,Removable locking dinkle connector with screw terminals & loop through facility,"C-Ring, tile-bridge kit, cut-out template, round white grille",1,1,"Steel, weather resistent coating (White)",Ø11.18"" (284mm),Grille Scrim - Black,Black Grille,294mm (11.55""),273.5mm (10.76""),62Hz-19kHz,50Hz-20kHz,118,116,112,0,1,0,Salt Spray & Chlorine,IP33,"Backcan: Powder Coated Steel (Black), Baffle: High Impact ABS UL-V0 (Black), Grille: Steel, weather resistent coating (White)",200.214603555827,0,100.000000000000,5.6,6"" Premium POE Ceiling Speaker (Blind Mount) - White,11.55078125,48,Ø 9.76"" (248mm),28,757,12,Steel - Black Powder coated,0,Ø  10.83"" (275.1mm)
FC-6D - White,13.2,https://www.atlasied.com,"Laminate, White, Matte","LF: (6"") 150mm Bass/Mid, mineral loaded polypropylene, HF: 1"" (25mm) titanium dome with neodymium magnet system, Ferrofluid cooled",7.125,PoE+ Type 2 / PoE++ Type 3 / PoE++ Type 4,"Dante, AES67",1,0,14.6"" x 33.7"" x 18.1"" (37cm x 85.5cm x 46cm),91,"UL2043, Conforms to UL62368-1, Certified to CSA STD 22.2 No. 62368-1                    EMC- FCC Part 15, Subpart B, EN 55032, EN 55035, EN IEC 6100, EN 6100",75,1,1.144059,https://www.atlasied.com/,,90,45,1,0,10,2,0,"Round black grill, square white grill, square black grill",-40°F to 140°F (-40° C to 60° C),FC-6D,150.16095266687,0,116,110,AtlasIED,5,Removable locking dinkle connector with screw terminals & loop through facility,"C-Ring, tile-bridge kit, cut-out template, round white grille",1,1,"Steel, weather resistent coating (White)",Ø11.18"" (284mm),Grille Scrim - White,White Grille,294mm (11.55""),273.5mm (10.76""),62Hz-19kHz,50Hz-20kHz,118,116,112,0,1,0,Salt Spray & Chlorine,IP33,"Backcan: Powder Coated Steel (Black), Baffle: High Impact ABS UL-V0 (Black), Grille: Steel, weather resistent coating (White)",200.214603555827,0,100.000000000000,5.6,6"" Premium POE Ceiling Speaker (Blind Mount) - White,11.55078125,48,Ø 9.76"" (248mm),28,757,12,Steel - Black Powder coated,0,Ø  10.83"" (275.1mm)
FC-4D - Black,7.9,https://www.atlasied.com,"Laminate, Black","LF: 4"" (100mm)  Bass/Mid, mineral loaded polypropylene, HF: 0.75"" (19mm) titanium dome with neodymium magnet system, Ferrofluid cooled",5.25,PoE+ Type 2 / PoE++ Type 3 / PoE++ Type 4,"Dante, AES67",1,0,11.8"" x 28"" x 14.6"" (30cm x 71cm x 37cm),88,"UL2043, Conforms to UL62368-1, Certified to CSA STD 22.2 No. 62368-1                    EMC- FCC Part 15, Subpart B, EN 55032, EN 55035, EN IEC 6100, EN 6100",75,1,2.282698,https://www.atlasied.com/,,90,45,1,0,10,2,0,"Round black grill, square white grill, square black grill",-40°F to 140°F (-40° C to 60° C),FC-4D,150.16095266687,0,112,106,AtlasIED,5,Removable locking dinkle connector with screw terminals & loop through facility,"C-Ring, tile-bridge kit, cut-out template, round white grille",1,1,"Steel, weather resistent coating (White)",Ø8.78"" (223mm),Grille Scrim - Black,Black Grille,8.91"" (226.5mm),8.13"" (206.5mm),80Hz-22kHz,62Hz-30kHz,118,116,112,0,0,1,Salt Spray & Chlorine,IP33,"Backcan: Powder Coated Steel (Black), Baffle: High Impact ABS UL-V0 (Black), Grille: Steel, weather resistent coating (White)",200.214603555827,0,100.000000000000,4.7,4"" Premium POE Ceiling Speaker (Blind Mount) - Black,8.91015625,48,Ø 7.56"" (192mm),28,757,12,Steel - Black Powder coated,0,Ø 8.42"" (213.9mm)
FC-4D - White,7.9,https://www.atlasied.com,"Laminate, White, Matte","LF: 4"" (100mm)  Bass/Mid, mineral loaded polypropylene, HF: 0.75"" (19mm) titanium dome with neodymium magnet system, Ferrofluid cooled",5.25,PoE+ Type 2 / PoE++ Type 3 / PoE++ Type 4,"Dante, AES67",1,0,11.8"" x 28"" x 14.6"" (30cm x 71cm x 37cm),88,"UL2043, Conforms to UL62368-1, Certified to CSA STD 22.2 No. 62368-1                    EMC- FCC Part 15, Subpart B, EN 55032, EN 55035, EN IEC 6100, EN 6100",75,1,2.282698,https://www.atlasied.com/,,90,45,1,0,10,2,0,"Round black grill, square white grill, square black grill",-40°F to 140°F (-40° C to 60° C),FC-4D,0,0,112,106,AtlasIED,5,Removable locking dinkle connector with screw terminals & loop through facility,"C-Ring, tile-bridge kit, cut-out template, round white grille",1,1,"Steel, weather resistent coating (White)",Ø8.78"" (223mm),Grille Scrim - White,White Grille,8.91"" (226.5mm),8.13"" (206.5mm),80Hz-22kHz,62Hz-30kHz,118,116,112,0,0,1,Salt Spray & Chlorine,IP33,"Backcan: Powder Coated Steel (Black), Baffle: High Impact ABS UL-V0 (Black), Grille: Steel, weather resistent coating (White)",0,0,0.000000000000,4.7,4"" Premium POE Ceiling Speaker (Blind Mount) - Black,8.91015625,48,Ø 7.56"" (192mm),28,757,12,Steel - Black Powder coated,0,Ø 8.42"" (213.9mm)
