,Weight (lbs)##OTHER##,URL##OTHER##,Transformer##OTHER##,Taps##OTHER##,Size##OTHER##,Sensativity##OTHER##,Outer material##OTHER##,Mounting type##OTHER##,Model##OTHER##,Manufacturer##OTHER##,Frequency Response##OTHER##,Dispersion##ANGLE##DEGREES,Description##OTHER##,Depth##OTHER##,Default Elevation##LENGTH##INCHES
VTF-157UCN,3.2,www.atlasied.com,70.7V,"15, 8, 4, 2",6"" square,96.9 dB @1W/1m,Aluminum_Neutral Gray,Flush mounted,VTF,Atlas,600Hz - 5500Hz (+/- 5dB),190.000000000000,Wall-mounted intercom loudspeaker,3 1/4"",48.000000000000
VTF-157UCR,3.2,www.atlasied.com,70.7V,"15, 8, 4, 2",6"" square,96.9 dB @1W/1m,Aluminum_Red,Flush mounted,VTF,Atlas,600Hz - 5500Hz (+/- 5dB),190.000000000000,Wall-mounted intercom loudspeaker,3 1/4"",48.000000000000
VTF-152UCR,3.2,www.atlasied.com,25V,"15, 8, 4, 2",6"" square,96.9 dB @1W/1m,Aluminum_Red,Flush mounted,VTF,Atlas,600Hz - 5500Hz (+/- 5dB),190.000000000000,Wall-mounted intercom loudspeaker,3 1/4"",48.000000000000
VTF-152UCN,3.2,www.atlasied.com,25V,"15, 8, 4, 2",6"" square,96.9 dB @1W/1m,Aluminum_Neutral Gray,Flush mounted,VTF,Atlas,600Hz - 5500Hz (+/- 5dB),190.000000000000,Wall-mounted intercom loudspeaker,3 1/4"",48.000000000000
