,Weight (lbs)##OTHER##,Vertical Coverage##ANGLE##DEGREES,URL##OTHER##,Transformer Taps##OTHER##,Sensativity (1W/1m)##OTHER##,SPL Max##OTHER##,Pitch##ANGLE##DEGREES,Mount Material##OTHER##,Model##OTHER##,Manufacturer##OTHER##,Input Connection##OTHER##,Ingress Protection##OTHER##,Impedance##OTHER##,Horizontal Coverage##ANGLE##DEGREES,Grille Material##OTHER##,Frequency Range##OTHER##,Enclosure Material##OTHER##,Default Elevation##LENGTH##INCHES,Coverage Cone##OTHER##
FS12T-66,48,60.000000000000,www.atlasied.com,"50, 100, 200, 400",102.5,128.5,45.000000000000,Steel - Gray epoxy,FS12T-66,AtlasIED,Barrier Terminal,IP45 When Tilted 5° Downwards,4,60.000000000000,Grille - Gray,80Hz - 17.6kHz (+/-5dB),Plastic - Battle Ship Gray,96,0
FS12T-99,48,90.000000000000,www.atlasied.com,"50, 100, 200, 400",102.5,128.5,0.000000000000,Steel - Gray epoxy,FS12T-99,AtlasIED,Barrier Terminal,IP45 When Tilted 5° Downwards,4,90.000000000000,Grille - Gray,80Hz - 17.6kHz (+/-5dB),Plastic - Battle Ship Gray,96,0
FS12T-94,48,40.000000000000,www.atlasied.com,"50, 100, 200, 400",102.5,128.5,0.000000000000,Steel - Gray epoxy,FS12T-94,AtlasIED,Barrier Terminal,IP45 When Tilted 5° Downwards,4,90.000000000000,Grille - Gray,80Hz - 17.6kHz (+/-5dB),Plastic - Battle Ship Gray,96,0
FS12T-BT60,39,90.000000000000,www.atlasied.com,"25, 50, 100, 200",93.5,116.5,0.000000000000,Steel - Gray epoxy,FS12T-BT60,AtlasIED,Barrier Terminal,IP45 When Tilted 5° Downwards,8,90.000000000000,Grille - Gray,62Hz - 14kHz (+/-5dB),Plastic - Battle Ship Gray,96,0
FS12T-SUB,41,179.000000000000,www.atlasied.com,"50, 100, 200, 400",96,124,0.000000000000,Steel - Gray epoxy,FS12T-SUB,AtlasIED,Barrier Terminal,IP45 When Tilted 5° Downwards,4,179.000000000000,Grille - Gray,47Hz - 130Hz (+/-5dB),Plastic - Battle Ship Gray,96,0
