,Weight (lbs)##OTHER##,Warranty##OTHER##,Vertical Symmetry##OTHER##,URL##OTHER##,Transformer Option##OTHER##,Speaker Listening Height##LENGTH##INCHES,Speaker Height##LENGTH##INCHES,Speaker Dispersion##ANGLE##DEGREES,Coverage Cone Visible##OTHER##,Sensitivity##OTHER##,SPL Max##OTHER##,Product Page URL##OTHER##,Product Documentation Link##OTHER##,Power Rating (RMS)##OTHER##,Pitch##ANGLE##DEGREES,OmniClass Title##OTHER##,OmniClass Number##OTHER##,Mount Material##OTHER##,Model##OTHER##,MaterFormat Title##OTHER##,MasterFormat##OTHER##,Market##OTHER##,Manufacturer URL##OTHER##,Manufacturer Phone##OTHER##,Manufacturer Email##OTHER##,Manufacturer Address##OTHER##,Manufacturer##OTHER##,Input Connectors##OTHER##,Ingress Protection##OTHER##,Impedance##OTHER##,IQ Category##OTHER##,Frequency Response ##OTHER##,Family Version##OTHER##,Family Code (default)##OTHER##,Enclosure Material##OTHER##,Dispersion Angle##ANGLE##DEGREES,Description##OTHER##,Default Elevation##LENGTH##INCHES,Cost##CURRENCY##CURRENCY,70V Taps##OTHER##,25V Taps##OTHER##,100V Taps##OTHER##
AP-30T,5,5 Year,1,www.atlassound.com,1,30.000000000000,120.000000000000,60.000000000000,0,108,121,https://www.atlasied.com/ap-30t,https://www.atlasied.com/f/643/ATS003854_AP-30_Series_Datasheet.pdf,30 Watts Continuous,-45.000000000000,SPEAKERS,23-37 17 13 19,Steel - Gray epoxy,AP-30T,SPEAKERS,27 41 13,"Commercial, Higher Education, Emergency",https://www.atlasied.com,(800) 876 - 3333,support@atlasied.com,"4545 E. Baseline Rd., Phoenix, AZ 85042",ATLAS SOUND,Barrier Terminal,IP-34,8,SPEAKERS,"300 - 12,000 Hz (Nominal) 500 Hz - 4500 Hz (±5dB)",2017-01,LOUD SPEAKERS,Steel - Gray epoxy,60.000000000000,HORN LOUDSPEAKER WITH 30-WATT 25V/70V/100V TRANSFORMER,48.000000000000,168.990000000000,"2, 3.8, 7.5, 15 and 30 watts",".9, 1.8, 3.7, 7.5 and 15 watts","4, 7.7, 15 and 30 Watts"
AP-30TC,5,5 Year,1,www.atlassound.com,1,30.000000000000,120.000000000000,60.000000000000,0,108,121,https://www.atlasied.com/ap-30t,https://www.atlasied.com/f/643/ATS003854_AP-30_Series_Datasheet.pdf,30 Watts Continuous,-45.000000000000,SPEAKERS,23-37 17 13 19,Steel - Beige epoxy,AP-30TC,SPEAKERS,27 41 13,"Commercial, Higher Education, Emergency",https://www.atlasied.com,(800) 876 - 3333,support@atlasied.com,"4545 E. Baseline Rd., Phoenix, AZ 85042",ATLAS SOUND,Barrier Terminal,IP-34,8,SPEAKERS,"300 - 12,000 Hz (Nominal) 500 Hz - 4500 Hz (±5dB)",2017-01,LOUD SPEAKERS,Steel - Beige epoxy,60.000000000000,HORN LOUDSPEAKER WITH 30-WATT 25V/70V/100V TRANSFORMER,48.000000000000,168.990000000000,"2, 3.8, 7.5, 15 and 30 watts",".9, 1.8, 3.7, 7.5 and 15 watts","4, 7.7, 15 and 30 Watts"
AP-30,4.5,5 Year,1,www.atlassound.com,0,30.000000000000,120.000000000000,60.000000000000,0,108,121,https://www.atlasied.com/ap-30t,https://www.atlasied.com/f/643/ATS003854_AP-30_Series_Datasheet.pdf,30 Watts Continuous,-45.000000000000,SPEAKERS,23-37 17 13 19,Steel - Gray epoxy,AP-30,SPEAKERS,27 41 13,"Commercial, Higher Education, Emergency",https://www.atlasied.com,(800) 876 - 3333,support@atlasied.com,"4545 E. Baseline Rd., Phoenix, AZ 85042",ATLAS SOUND,Barrier Terminal,IP-34,8,SPEAKERS,"300 - 12,000 Hz (Nominal) 500 Hz - 4500 Hz (±5dB)",2017-01,LOUD SPEAKERS,Steel - Gray epoxy,60.000000000000,HORN LOUDSPEAKER WITH 30-WATT 25V/70V/100V TRANSFORMER,48.000000000000,168.990000000000,"2, 3.8, 7.5, 15 and 30 watts",".9, 1.8, 3.7, 7.5 and 15 watts","4, 7.7, 15 and 30 Watts"
