,Weight (lbs)##OTHER##,URL##OTHER##,Transformer Taps##OTHER##,Tile Rails##OTHER##,New Construction Ring##OTHER##,Standard Grille##OTHER##,Speaker Type Visible##OTHER##,Speaker Type Annotation##OTHER##,Sensitivity##OTHER##,SPL Target##OTHER##,REP##OTHER##,Peak Factor##OTHER##,Mount Material##OTHER##,Model##OTHER##,Minimum Tap##OTHER##,Minimum Overlap Guide##OTHER##,Manufacturer##OTHER##,Listener Height##LENGTH##INCHES,Ingress Protection##OTHER##,Grille Scrim Material##OTHER##,Grille Material##OTHER##,Frequency Response##OTHER##,Enclosure Material##OTHER##,Edgeless Square Grille##OTHER##,Edgeless Round Grille##OTHER##,Edge-To-Edge Guide##OTHER##,Doglegs Stowed##OTHER##,Dispersion##ANGLE##DEGREES,Description##OTHER##,Default Elevation##LENGTH##INCHES,Dispersion Cone Depth##LENGTH##INCHES,Dispersion Cone##OTHER##,Certifications##OTHER##,Ceiling Thickness##LENGTH##INCHES,Ceiling Height##LENGTH##INCHES,C-Ring##OTHER##,Baffle Material##OTHER##
FAP33T-W,4.14,www.atlasied.com,"2W, 4W, 8W, 16W",1,0,1,0,S1,89,75,1.813211,10,Plastic - White - Smooth,FAP33T-W,2,0,AtlasIED,5,IP-21,Grille Scrim - White,Grille - White,110Hz - 12kHz (+/- 5dB),Steel - Gray epoxy,0,0,0,0,105.000000000000,Full Range Ceiling Loudspeaker,48,84,0,"UL1480, UL2043 and CSA C22.2 No. 205.",0.5,12,1,Plastic - White - Smooth
FAP33T-W + Round Edgeless Grille EGR33W (White),4.14,www.atlasied.com,"2W, 4W, 8W, 16W",1,0,0,0,S1,89,75,1.813211,10,Plastic - White - Smooth,FAP33T-W + Round Edgeless Grille EGR33W,2,0,AtlasIED,5,IP-21,Grille Scrim - White,Grille - White,110Hz - 12kHz (+/- 5dB),Steel - Gray epoxy,0,1,0,0,105.000000000000,Full Range Ceiling Loudspeaker,48,84,0,"UL1480, UL2043 and CSA C22.2 No. 205.",0.5,12,1,Plastic - White - Smooth
FAP33T-W + Square Edgeless Grille EGS33W (White),4.14,www.atlasied.com,"2W, 4W, 8W, 16W",1,0,0,0,S1,89,75,1.813211,10,Plastic - White - Smooth,FAP33T-W + Square Edgeless Grille EGS33W,2,0,AtlasIED,5,IP-21,Grille Scrim - White,Grille - White,110Hz - 12kHz (+/- 5dB),Steel - Gray epoxy,1,0,0,0,105.000000000000,Full Range Ceiling Loudspeaker,48,84,0,"UL1480, UL2043 and CSA C22.2 No. 205.",0.5,12,1,Plastic - White - Smooth
FAP33T-W + Round Edgeless Grille EGR33B (Black),4.14,www.atlasied.com,"2W, 4W, 8W, 16W",1,0,0,0,S1,89,75,1.813211,10,Plastic - White - Smooth,FAP33T-W + Round Edgeless Grille EGR33B,2,0,AtlasIED,5,IP-21,Grille Scrim - Black,Grille - Black,110Hz - 12kHz (+/- 5dB),Steel - Gray epoxy,0,1,0,0,105.000000000000,Full Range Ceiling Loudspeaker,48,84,0,"UL1480, UL2043 and CSA C22.2 No. 205.",0.5,12,1,Plastic - White - Smooth
FAP33T-W + Square Edgeless Grille EGS33B (Black),4.14,www.atlasied.com,"2W, 4W, 8W, 16W",1,0,0,0,S1,89,75,1.813211,10,Plastic - White - Smooth,FAP33T-W + Square Edgeless Grille EGS33B,2,0,AtlasIED,5,IP-21,Grille Scrim - Black,Grille - Black,110Hz - 12kHz (+/- 5dB),Steel - Gray epoxy,1,0,0,0,105.000000000000,Full Range Ceiling Loudspeaker,48,84,0,"UL1480, UL2043 and CSA C22.2 No. 205.",0.5,12,1,Plastic - White - Smooth
