,Weight (lbs)##OTHER##,URL##OTHER##,Transformer Taps##OTHER##,Tile Bridges##OTHER##,Speaker Type Visible##OTHER##,Speaker Type Annotation##OTHER##,Sensitivity##OTHER##,SPL Target##OTHER##,REP##OTHER##,Peak Factor##OTHER##,New Construction Ring##OTHER##,Mount Material##OTHER##,Model##OTHER##,Minimum Tap##OTHER##,Minimum Overlap Guide##OTHER##,Manufacturer##OTHER##,Listener Height##LENGTH##INCHES,Ingress Protection##OTHER##,Grille Scrim Material##OTHER##,Grille Material##OTHER##,Grille - Standard##OTHER##,Grille - Square Edgeless##OTHER##,Grille - Round Edgeless##OTHER##,Frequency Response##OTHER##,Enclosure Material##OTHER##,Edge-To-Edge Guide##OTHER##,Doglegs Stowed##OTHER##,Dispersion Cone Visible##OTHER##,Dispersion Cone Height##LENGTH##INCHES,Dispersion##ANGLE##DEGREES,Description##OTHER##,Default Elevation##LENGTH##INCHES,Certifications##OTHER##,Ceiling Thickness##LENGTH##INCHES,Ceiling Height##LENGTH##INCHES,C-Ring##OTHER##,Baffle Material##OTHER##
FAP43T-W,6.23,www.atlasied.com,"4W, 8W, 16W, 32W",1,0,S1,90,75,1.440285,10,0,Plastic - White - Smooth,FAP43T-W,4,0,AtlasIED,5,IP-21,Grille Scrim - White,Grille - White,1,0,0,90Hz - 20kHz (+/- 5dB),Steel - Gray epoxy,0,0,0,84,130.000000000000,Full Range Ceiling Loudspeaker,48,"UL1480, UL2043 and CSA C22.2 No. 205",0.5,12,1,Plastic - White - Smooth
FAP43T-W + EGR43W (White),6.23,www.atlasied.com,"4W, 8W, 16W, 32W",1,0,S1,90,75,1.440285,10,0,Plastic - White - Smooth,FAP43T-W + EGR43W,4,0,AtlasIED,5,IP-21,Grille Scrim - White,Grille - White,0,0,1,90Hz - 20kHz (+/- 5dB),Steel - Gray epoxy,0,0,0,84,130.000000000000,Full Range Ceiling Loudspeaker,48,"UL1480, UL2043 and CSA C22.2 No. 205",0.5,12,1,Plastic - White - Smooth
FAP43T-W + EGS43W (White),6.23,www.atlasied.com,"4W, 8W, 16W, 32W",1,0,S1,90,75,1.440285,10,0,Plastic - White - Smooth,FAP43T-W + EGS43W,4,0,AtlasIED,5,IP-21,Grille Scrim - White,Grille - White,0,1,0,90Hz - 20kHz (+/- 5dB),Steel - Gray epoxy,0,0,0,84,130.000000000000,Full Range Ceiling Loudspeaker,48,"UL1480, UL2043 and CSA C22.2 No. 205",0.5,12,1,Plastic - White - Smooth
FAP43T-W + EGR43B (Black),6.23,www.atlasied.com,"4W, 8W, 16W, 32W",1,0,S1,90,75,1.440285,10,0,Plastic - White - Smooth,FAP43T-W + EGR43B,4,0,AtlasIED,5,IP-21,Grille Scrim - Black,Grille - Black,0,0,1,90Hz - 20kHz (+/- 5dB),Steel - Gray epoxy,0,0,0,84,130.000000000000,Full Range Ceiling Loudspeaker,48,"UL1480, UL2043 and CSA C22.2 No. 205",0.5,12,1,Plastic - White - Smooth
FAP43T-W + EGS43W (Black),6.23,www.atlasied.com,"4W, 8W, 16W, 32W",1,0,S1,90,75,1.440285,10,0,Plastic - White - Smooth,FAP43T-W + EGS43B,4,0,AtlasIED,5,IP-21,Grille Scrim - Black,Grille - Black,0,1,0,90Hz - 20kHz (+/- 5dB),Steel - Gray epoxy,0,0,0,84,130.000000000000,Full Range Ceiling Loudspeaker,48,"UL1480, UL2043 and CSA C22.2 No. 205",0.5,12,1,Plastic - White - Smooth
